{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTY-HL"]
[]
[]
[]
[]
["","","","","","FTY18HEVLK","FTY24HEVLK","FTY30HEVLK"]
["Sound pressure level","Heating","","High","dBA","44","45"]
["","","","Silent operation","dBA","35","32"]
["","","","Low","dBA","38","37"]
["","Cooling","","Silent operation","dBA","33","34"]
["","","","Low","dBA","36","37"]
["","","","High","dBA","44","45"]
["","","","Nom.","dBA","40","40","44"]
["","Cooling","","Nom.","dBA","40","42","44"]
["Dimensions","Unit","","Width","mm","940","1,007","1,178"]
["","","","Depth","mm","298","219","227"]
["","","","Height","mm","200","315","326"]
["Weight","Unit","","","kg","13","15.5","17.5"]
["Fan","Air flow rate","Heating","High","m³/min","780","800"]
["","","","Low","m³/min","550","600"]
["","","Cooling","Low","m³/min","550","600"]
["","","","High","m³/min","780","800"]
["","","","Nom.","m³/min","650","700"]
["","","Cooling","Nom.","m³/min","650","700"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Name","","","","VL","VL","VL"]
["","Frequency","","","Hz","60","60","60"]
["","Voltage","","","V","220","220","220"]