{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTYD-JVL / RYD-JVL/JTL/JYL"]
[]
[]
[]
[]
["","","","","FTYD20JEVLK / RYD20JEVLK","FTYD25JEVLK / RYD25JEVLK"]
["Cooling capacity","Nom.","","kW","5.570 (3)","6.650 (3)"]
["Piping connections","Liquid","OD","mm","6.35","9.52"]
["","Gas","OD","mm","15.88","15.88"]
["Nominal efficiency","EER","","","2.90","2.73"]
["","Annual energy consumption","","kWh","960","1,220"]
["","COP","","","3.10","3.03"]
["","Energy labeling Directive","Cooling","","C","D"]
["","","Heating","","D","D"]
["Heating capacity","Nom.","","kW","5.860 (4)","7.03 (4)"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB","(4) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB"]
["","","","","(5) - Heating: indoor temp. 20°CDB; outdoor temp. 8°CDB, 6°CWB","(5) - Heating: indoor temp. 20°CDB; outdoor temp. 8°CDB, 6°CWB"]
["","","","","(6) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(6) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit)."]
["","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]