{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTYD-JVL"]
[]
[]
[]
[]
["","","","","FTYD20JEVLK","FTYD25JEVLK"]
["Sound pressure level","Heating","High","dBA","42","45"]
["","","Silent operation","dBA","35","37"]
["","","Low","dBA","36","40"]
["","Cooling","Silent operation","dBA","35","37"]
["","","Super high","dBA","44","46"]
["","","Low","dBA","36","40"]
["","","High","dBA","42","45"]
["","","Nom.","dBA","39","43"]
["","Cooling","Nom.","dBA","39","43"]
["Dimensions","Unit","Width","mm","1,065","1,065"]
["","","Depth","mm","228","228"]
["","","Height","mm","310","310"]
["Casing","Colour","","","White","White"]
["Weight","Unit","","kg","14","14"]
["Fan","External static pressure","Nom.","Pa","0","0"]
["Power supply","Phase","","","1~","1~"]
["","Frequency","","Hz","60","60"]
["","Voltage","","V","220","220"]