{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZQG100L8Y1B","FVA140AMVEB / RZQG100L8Y1B","FVA140AMVEB / RZQG125L8Y1B","FVA100AMVEB / RZQG71L8Y1B","FVA71AMVEB / RZQG71L8Y1B","FVA125AMVEB / RZQG125L8Y1B","FVA140AMVEB / RZQG140L7Y1B"]
["Cooling capacity","Nom.","","kW","","","","6.80","6.80","12.00","13.40"]
["Space cooling","SEER","","","","","","6.23","6.23","5.61","5.89"]
["","ηs,c","","%","","","","","","","232.61"]
["","Annual energy consumption","","kWh/a","","","","383","383","749","1,365"]
["","Capacity","Pdesign","kW","","","","6.80","6.80","12.00","13.40"]
["","Energy efficiency class","","","","","","A++","A++","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","6.33","6.33","11.30","11.47"]
["","SCOP/A","","","","","","4.05","4.05","3.87","3.88"]
["","Energy efficiency class","","","","","","A+","A+","A"]
["","Annual energy consumption","","kWh/a","","","","2,189","2,189","4,088","4,132"]
["","ηs,h","","%","","","","","","","152.39"]
["Nominal efficiency","EER","","","","","","3.37","3.37","3.21","2.79"]
["","Annual energy consumption","","kWh","","","","","1,009","1,869"]
["","COP","","","","","","","3.64","3.70","3.61"]
["","Energy labeling Directive","Cooling","","","","","","A","A"]
["","","Heating","","","","","","A","A"]
["Heating capacity","Nom.","","kW","","","","","7.50","13.50","15.50"]
["Notes","","","","","","","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]