{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":12,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXCQ-MVE"]
[]
[]
[]
[]
["","","","","FXCQ20MVE9","FXCQ25MVE9","FXCQ32MVE9","FXCQ40MVE9","FXCQ50MVE9","FXCQ63MVE9","FXCQ80MVE9","FXCQ125MVE9"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Paper pattern for installation","","","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation"]
["","Washer for hanger bracket","","","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket"]
["","Clamp metal","","","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal"]
["","Drain hose","","","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Washer fixing plate","","","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate"]
["","Sealing pads","","","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads"]
["","Clamps","","","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps"]
["","Screws","","","Screws","Screws","Screws","Screws","Screws","Screws","Screws","Screws"]
["","Washer","","","Washer","Washer","Washer","Washer","Washer","Washer","Washer","Washer"]
["Refrigerant","Type","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","9.52","9.52","9.52"]
["","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","OD","mm","12.7","12.7","12.7","12.7","12.7","15.9","15.9","15.9"]
["","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Dimensions","Unit","Width","mm","775","775","775","990","990","1,175","1,665","1,665"]
["","","Depth","mm","600","600","600","600","600","600","600","600"]
["","","Height","mm","305","305","305","305","305","305","305","305"]
["Casing","Material","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","kg","26","26","26","31","32","35","47","48"]
["Decoration panel","Weight","","kg","8","8","8","8.5","8.5","9.5","12","12"]
["","Model","","","BYBC32GJW1, BYBC32G-W1","BYBC32GJW1, BYBC32G-W1","BYBC32GJW1, BYBC32G-W1","BYBC50GJW1, BYBC50G-W1","BYBC50GJW1, BYBC50G-W1","BYBC63GJW1, BYBC63G-W1","BYBC125GJW1, BYBC125G-W1","BYBC125GJW1, BYBC125G-W1"]
["","Dimensions","Height","mm","53","53","53","53","53","53","53","53"]
["","","Depth","mm","680","680","680","680","680","680","680","680"]
["","","Width","mm","1,030","1,030","1,030","1,245","1,245","1,430","1,920","1,920"]
["","Colour","","","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)","White (10Y9/0.5)"]
["Current - 50Hz","Maximum fuse amps (MFA)","","A","15","15","15","15","15","15","15","15"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","VE","VE","VE","VE","VE","VE","VE","VE"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)"]
["","","","","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","(6) - MCA/MFA: MCA = 1.25 x FLA","(6) - MCA/MFA: MCA = 1.25 x FLA","(6) - MCA/MFA: MCA = 1.25 x FLA","(6) - MCA/MFA: MCA = 1.25 x FLA","(6) - MCA/MFA: MCA = 1.25 x FLA","(6) - MCA/MFA: MCA = 1.25 x FLA","(6) - MCA/MFA: MCA = 1.25 x FLA","(6) - MCA/MFA: MCA = 1.25 x FLA"]
["","","","","(7) - MFA ≤ 4 x FLA","(7) - MFA ≤ 4 x FLA","(7) - MFA ≤ 4 x FLA","(7) - MFA ≤ 4 x FLA","(7) - MFA ≤ 4 x FLA","(7) - MFA ≤ 4 x FLA","(7) - MFA ≤ 4 x FLA","(7) - MFA ≤ 4 x FLA"]
["","","","","(8) - Next lower standard fuse rating minimum 15A","(8) - Next lower standard fuse rating minimum 15A","(8) - Next lower standard fuse rating minimum 15A","(8) - Next lower standard fuse rating minimum 15A","(8) - Next lower standard fuse rating minimum 15A","(8) - Next lower standard fuse rating minimum 15A","(8) - Next lower standard fuse rating minimum 15A","(8) - Next lower standard fuse rating minimum 15A"]
["","","","","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA","(9) - Select wire size based on the value of MCA"]
["","","","","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker"]