{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":12,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXFQ-PV9"]
[]
[]
[]
[]
["","","","","FXFQ25PVE9","FXFQ32PVE9","FXFQ40PVE9","FXFQ50PVE9","FXFQ63PVE9","FXFQ80PVE9","FXFQ100PVE9","FXFQ125PVE9"]
["Sound pressure level","Cooling","Super high","dBA","30.0","30.0","31.0","32.0","34.0","36.0","44.0","44.0"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Paper pattern for installation","","","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation"]
["","Drain hose","","","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Clamp metal","","","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal"]
["","Washer fixing plate","","","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate"]
["","Sealing pads","","","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads"]
["","Clamps","","","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps"]
["","Screws","","","Screws","Screws","Screws","Screws","Screws","Screws","Screws","Screws"]
["","Washer for hanger bracket","","","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Installation guide","","","Installation guide","Installation guide","Installation guide","Installation guide","Installation guide","Installation guide","Installation guide","Installation guide"]
["Refrigerant","Type","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","OD","mm","12.7","12.7","12.7","12.7","15.9","15.9","15.9","15.9"]
["","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Dimensions","Unit","Width","mm","840","840","840","840","840","840","840","840"]
["","","Depth","mm","840","840","840","840","840","840","840","840"]
["","","Height","mm","246","246","246","246","246","246","288","288"]
["Casing","Material","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","kg","19.5","19.5","19.5","19.5","22","22","25","25"]
["Decoration panel","Weight","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["","Model","","","BYC125K-W1","BYC125K-W1","BYC125K-W1","BYC125K-W1","BYC125K-W1","BYC125K-W1","BYC125K-W1","BYC125K-W1"]
["","Dimensions","Height","mm","50","50","50","50","50","50","50","50"]
["","","Depth","mm","950","950","950","950","950","950","950","950"]
["","","Width","mm","950","950","950","950","950","950","950","950"]
["","Colour","","","Fresh white (6.5Y 9.5/0.5)","Fresh white (6.5Y 9.5/0.5)","Fresh white (6.5Y 9.5/0.5)","Fresh white (6.5Y 9.5/0.5)","Fresh white (6.5Y 9.5/0.5)","Fresh white (6.5Y 9.5/0.5)","Fresh white (6.5Y 9.5/0.5)","Fresh white (6.5Y 9.5/0.5)"]
["Current - 50Hz","Maximum fuse amps (MFA)","","A","15","15","15","15","15","15","15","15"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","VE","VE","VE","VE","VE","VE","VE","VE"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m (horizontal)"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m (horizontal)"]
["","","","","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","(4) - Operation sound differs with operation and ambient conditions","(4) - Operation sound differs with operation and ambient conditions","(4) - Operation sound differs with operation and ambient conditions","(4) - Operation sound differs with operation and ambient conditions","(4) - Operation sound differs with operation and ambient conditions","(4) - Operation sound differs with operation and ambient conditions","(4) - Operation sound differs with operation and ambient conditions","(4) - Operation sound differs with operation and ambient conditions"]
["","","","","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA"]
["","","","","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA"]
["","","","","(9) - Next lower standard fuse rating minimum 15A","(9) - Next lower standard fuse rating minimum 15A","(9) - Next lower standard fuse rating minimum 15A","(9) - Next lower standard fuse rating minimum 15A","(9) - Next lower standard fuse rating minimum 15A","(9) - Next lower standard fuse rating minimum 15A","(9) - Next lower standard fuse rating minimum 15A","(9) - Next lower standard fuse rating minimum 15A"]
["","","","","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA"]
["","","","","(11) - Instead of a fuse, use a circuit breaker","(11) - Instead of a fuse, use a circuit breaker","(11) - Instead of a fuse, use a circuit breaker","(11) - Instead of a fuse, use a circuit breaker","(11) - Instead of a fuse, use a circuit breaker","(11) - Instead of a fuse, use a circuit breaker","(11) - Instead of a fuse, use a circuit breaker","(11) - Instead of a fuse, use a circuit breaker"]