{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":136,"n_cols":14,"rows_kept":136,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHSCU-CL3"]
[]
[]
[]
[]
["","","","","","JEHSCU0300CL3","JEHSCU0400CL3","JEHSCU0500CL3","JEHSCU0600CL3","JEHSCU0750CL3","JEHSCU0950CL3 EVI","JEHSCU0951CL3 EVI","JEHSCU0951CL3 EVI_","JEHSCU0200CL3 (Archived)"]
["Refrigerating capacity","Low temperature","R-448A","Nom","kW","1.62","2.53","","3.49","4.81"]
["","","R-449A","Nom","kW","1.62","2.53","","3.49","4.81"]
["","","R-407F","Nom","kW","","2.38","2.87","","","4.88"]
["","","R-407A","Nom","kW","","2.29","2.77","3.31","","4.96"]
["Annual electricity consumption Q","R-407A","","Te -35°C","kWh/a","","10,212.00","12,364.00","15,026.00","","20,958.00"]
["","R-449A","","Te -35°C","kWh/a","","11,276.00","","15,878.00","21,856.00"]
["","R-448A","","Te -35°C","kWh/a","","11,276.00","","15,878.00","21,856.00"]
["","R-407F","","Te -35°C","kWh/a","","10,730.00","13,018.00","","","22,348.00"]
["Parameters at full load and ambient temp. 43°C","R-449A","Te -35°C","Power input (D3)","kW","2.11","3.29","","6.15","5.28"]
["","","","Cooling capacity (P3)","kW","1.43","2.23","","2.82","4.26"]
["","R-407A","Te -35°C","Cooling capacity (P3)","kW","","2.01","2.40","2.88"]
["","","","Declared COP (COP3)","","","0.67","0.66","0.64"]
["","","","Power input (D3)","kW","","2.98","3.64","4.48"]
["","R-407F","Te -35°C","Power input (D3)","kW","","3.30"]
["","","","Cooling capacity (P3)","kW","","2.04"]
["","","","Declared COP (COP3)","","","0.62"]
["","R-404A","Te -35°C","Declared COP (COP3)","","","","","","","","","","0.60"]
["","R-448A","Te -35°C","Power input (D3)","kW","2.11","3.29","","6.15","5.28"]
["","","","Cooling capacity (P3)","kW","1.43","2.23","","2.82","4.26"]
["Weight","Unit","","","kg","78","132","132","133","203","200","","","76"]
["Parameters at full load and ambient temp. 25°C","R-449A","Te -35°C","Power input (D2)","kW","1.48"]
["","","","Cooling capacity (P2)","kW","1.71"]
["","R-404A","Te -35°C","Declared COP (COP2)","","","","","","","","","","1.16"]
["","R-448A","Te -35°C","Cooling capacity (P2)","kW","1.71"]
["","","","Power input (D2)","kW","1.48"]
["Seasonal energy performance ratio SEPR","R-407F","","Te -35°C","","","1.65","1.64","","","1.63"]
["","R-407A","","Te -35°C","","","1.67","1.67","1.64","","1.76"]
["Refrigerant","GWP Type 5","","","","1,387","1,387","","1,387","1,387","1,387"]
["","GWP Type 2","","","","","2,107","2,107","2,107","","2,107"]
["","GWP Type 3","","","","","1,825","1,825","","","1,825"]
["","GWP","","","","","","","","","","","","3,922"]
["","Type 3","","","","","R-407F","R-407F","","","R-407F"]
["","Type 2","","","","","R-407A","R-407A","R-407A","","R-407A"]
["","Type 5","","","","R-448A","R-448A","","R-448A","R-448A","R-448A"]
["","Type","","","","","","","","","","","","R-404A"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-404A","Te -35°C","Rated COP (COPA)","","","","","","","","","","0.97"]
["","","","Rated  power input (DA)","kW","","","","","","","","","1.46"]
["","","","Rated  cooling capacity (PA)","kW","","","","","","","","","1.42"]
["","R-448A","Te -35°C","Rated  power input (DA)","kW","1.67","2.48","","4.19","4.08"]
["","","","Rated  cooling capacity (PA)","kW","1.62","2.53","","3.49","4.81"]
["","R-407F","Te -35°C","Rated  power input (DA)","kW","","2.51","3.08","","","4.51"]
["","","","Rated COP (COPA)","","","0.95","0.93","","","1.08"]
["","","","Rated  cooling capacity (PA)","kW","","2.38","2.87","","","4.88"]
["","R-407A","Te -35°C","Rated COP (COPA)","","","0.98","0.97","0.93","","1.26"]
["","","","Rated  cooling capacity (PA)","kW","","2.29","2.77","3.31","","4.96"]
["","","","Rated  power input (DA)","kW","","2.33","2.85","3.57","","3.94"]
["","R-449A","Te -35°C","Rated  cooling capacity (PA)","kW","1.62","2.53","","3.49","4.81"]
["","","","Rated  power input (DA)","kW","1.67","2.48","","4.19","4.08"]
["Power input","Low temperature","R-407A","Nom","kW","","2.33","2.85","3.57","","3.94"]
["","","R-448A","Nom","kW","1.67","2.48","","4.19","4.08"]
["","","R-449A","Nom","kW","1.67","2.48","","4.19","4.08"]
["COP","Low temperature","","R-407F","","","0.95","0.93","","","1.08"]
["","","","R-407A","","","0.98","0.97","0.93","","1.26"]
["Dimensions","Unit","","Width","mm","1,101","1,353","1,353","1,353","1,348","1,348","","","1,101"]
["","","","Depth","mm","444","575","575","575","605","605","","","444"]
["","","","Height","mm","662","872","872","872","1,727","1,727","","","662"]
["Casing","Colour","","","","Light grey","Light grey","Light grey","Light grey","Light grey","Light grey","","","Light grey"]
["Fan","Type","","","","Axial","Axial","Axial","Axial","Axial","Axial","","","Axial"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~","3~","","","3~"]
["","Frequency","","","Hz","50","50","50","50","50","50","","","50"]
["","Voltage","","","V","400","400","400","400","400","400","","","400"]
["Notes","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - Refer to condition: Outside ambient temperature = 32°C, Evaporation temperature = -10°C and 10K superheat (medium temperature application)","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room","","","(2) - Sound pressure level is measured at 10m in anechoic room"]
["","","","","","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","(3) - Its functioning relies on fluorinated greenhouse gases","","","(3) - Its functioning relies on fluorinated greenhouse gases"]
["Parameters at full load and ambient temp. 43°C","R-449A","Te -35°C","Declared COP (COP3)","","0.68","0.68","","0.46","0.81"]
["","R-448A","Te -35°C","Declared COP (COP3)","","0.68","0.68","","0.46","0.81"]
["Parameters at full load and ambient temp. 25°C","R-449A","Te -35°C","Declared COP (COP2)","","1.16"]
["","R-448A","Te -35°C","Declared COP (COP2)","","1.16"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-448A","Te -35°C","Rated COP (COPA)","","0.97","1.02","","0.83","1.18"]
["","R-449A","Te -35°C","Rated COP (COPA)","","0.97","1.02","","0.83","1.18"]
["COP","Low temperature","","R-449A","","0.97","1.02","","0.83","1.18"]
["","","","R-448A","","0.97","1.02","","0.83","1.18"]
["Seasonal energy performance ratio SEPR","R-448A","","Te -35°C","","","1.67","","1.64","1.64"]
["","R-449A","","Te -35°C","","","1.67","","1.64","1.64"]
["Refrigerating capacity","Low temperature","R-407A","Nom","kW","","","","","","","4.89","4.89"]
["","","R-407F","Nom","kW","","","","","","","4.90","4.90"]
["","","R-448A","Nom","kW","","","","","","","4.85","4.85"]
["","","R-449A","Nom","kW","","","","","","","4.85","4.85"]
["Power input","Low temperature","R-407A","Nom","kW","","","","","","","4.15","4.15"]
["","","R-407F","Nom","kW","","","","","","","3.86","3.86"]
["","","R-448A","Nom","kW","","","","","","","3.95","3.95"]
["","","R-449A","Nom","kW","","","","","","","3.95","3.95"]
["COP","Low temperature","","R-407A","","","","","","","","1.18","1.18"]
["","","","R-407F","","","","","","","","1.27","1.27"]
["","","","R-448A","","","","","","","","1.23","1.23"]
["","","","R-449A","","","","","","","","1.23","1.23"]
["Annual electricity consumption Q","R-407A","","Te -35°C","kWh/a","","","","","","","22108.00","22108.00"]
["","R-407F","","Te -35°C","kWh/a","","","","","","","20961.00","20961.00"]
["","R-448A","","Te -35°C","kWh/a","","","","","","","21477.00","21477.00"]
["","R-449A","","Te -35°C","kWh/a","","","","","","","21477.00","21477.00"]
["Seasonal energy performance ratio SEPR","R-407A","","Te -35°C","","","","","","","","1.65","1.65"]
["","R-407F","","Te -35°C","","","","","","","","1.74","1.74"]
["","R-448A","","Te -35°C","","","","","","","","1.68","1.68"]
["","R-449A","","Te -35°C","","","","","","","","1.68","1.68"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-407A","Te -35°C","Rated  cooling capacity (PA)","kW","","","","","","","4.89","4.89"]
["","","","Rated  power input (DA)","kW","","","","","","","3.15","3.15"]
["","","","Rated COP (COPA)","","","","","","","","1.18","1.18"]
["","R-407F","Te -35°C","Rated  cooling capacity (PA)","kW","","","","","","","4.90","4.90"]
["","","","Rated  power input (DA)","kW","","","","","","","3.86","3.86"]
["","","","Rated COP (COPA)","","","","","","","","1.27","1.27"]
["","R-448A","Te -35°C","Rated  cooling capacity (PA)","kW","","","","","","","4.85","4.85"]
["","","","Rated  power input (DA)","kW","","","","","","","3.95","3.95"]
["","","","Rated COP (COPA)","","","","","","","","1.23","1.23"]
["","R-449A","Te -35°C","Rated  cooling capacity (PA)","kW","","","","","","","4.85","4.85"]
["","","","Rated  power input (DA)","kW","","","","","","","3.95","3.95"]
["","","","Rated COP (COPA)","","","","","","","","1.23","1.23"]
["Casing","Colour","","","","","","","","","","Light grey","Light grey"]
["Dimensions","Unit","","Height","mm","","","","","","","1727","1727"]
["","","","Width","mm","","","","","","","1348","1348"]
["","","","Depth","mm","","","","","","","605","605"]
["Weight","Unit","","","kg","","","","","","","200","200"]
["Fan","Type","","","","","","","","","","Axial","Axial"]
["Refrigerant","Type 2","","","","","","","","","","R-407A","R-407A"]
["","Type 3","","","","","","","","","","R-407F","R-407F"]
["","Type 5","","","","","","","","","","R-448A","R-448A"]
["","GWP Type 2","","","","","","","","","","2107","2107"]
["","GWP Type 3","","","","","","","","","","1825","1825"]
["","GWP Type 5","","","","","","","","","","1387","1387"]
["Power supply","Phase","","","","","","","","","","3~","3~"]
["","Frequency","","","Hz","","","","","","","50","50"]
["","Voltage","","","V","","","","","","","400","400"]
["Unit","Nominal running current (RLA)","R-448A","Cooling","A","","","","","","","8.50","8.50"]
["","","R-449A","Cooling","A","","","","","","","8.50","8.50"]
["Notes","","","","","","","","","","","(2) - Sound pressure level is measured at 10m in anechoic room","(2) - Sound pressure level is measured at 10m in anechoic room"]
["Annual electricity consumption Q","R-404A","","Te -35°C","kWh/a","","","","","","","","24503"]
["Seasonal energy performance ratio SEPR","R-404A","","Te -35°C","","","","","","","","","1.79"]
["Parameters at full load and ambient temp. 32°C (Point A)","R-404A","Te -35°C","Rated  cooling capacity (PA)","kW","","","","","","","","5.90"]
["","","","Rated  power input (DA)","kW","","","","","","","","4.35"]
["","","","Rated COP (COPA)","","","","","","","","","1.36"]
["Parameters at full load and ambient temp. 43°C","R-404A","Te -35°C","Declared COP (COP3)","","","","","","","","","1.06"]