{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC707"]
[]
[]
[]
[]
["","","","","","MC707VM-S","MC707VM-W"]
["Sound pressure level","Air purifying operation","","High","dBA","38.0","38.0"]
["","","","Turbo","dBA","47.0","47.0"]
["","","","Medium","dBA","31.0","31.0"]
["","","","Low","dBA","24.0","24.0"]
["","","","Silent","dBA","16.0","16.0"]
["Standard Accessories","Infrared remote control","","","","1","Infrared remote control"]
["","Photocatalytic pleated Filter","","","","7","7"]
["","Operation manual","","","","1","1"]
["","Bio-antibody Filter","","","","1","1"]
["Safety devices","Item","","01","","Safety switch (operation stops when the front panel opens)","Safety switch (operation stops when the front panel opens)"]
["Dimensions","Unit","","Width","mm","425","425"]
["","","","Depth","mm","213","213"]
["","","","Height","mm","533","533"]
["Bacteria filtering method","","","","","Titanium apatite photocatalytic filter, Bio-antibody filter, Flash streamer","Titanium apatite photocatalytic filter, Bio-antibody filter, Flash streamer"]
["Casing","Colour","","","","Silver","White"]
["Applicable room area","m²","","","","48","48"]
["Dust collecting method","","","","","Electrostatic dust collection filter, Plasma ionizer (electrostatic dust collection)","Electrostatic dust collection filter, Plasma ionizer (electrostatic dust collection)"]
["Deodorizing method","","","","","Deodorising catalyst, Titanium apatite photocatalytic filter, Flash streamer","Deodorising catalyst, Flash streamer, Titanium apatite photocatalytic filter"]
["Weight","Unit","","","kg","8.7","8.7"]
["Type","","","","","Photocatalytic Air Purifier","Photocatalytic Air Purifier"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","420","420"]
["","","","High","m³/h","285","285"]
["","","","Silent","m³/h","60","60"]
["","","","Low","m³/h","120","120"]
["","","","Medium","m³/h","180","180"]
["Air flow control","Stages","","","","5","5"]
["Capacity","m³/min","","","","7.0","7.0"]
["Application","","","","","Desktop Type","Desktop Type"]
["Air purifying operation","Power input","","Turbo","kW","0.055","0.055"]
["","","","Silent","kW","0.008","0.008"]
["","","","L","kW","0.010","0.010"]
["","","","H","kW","0.023","0.023"]
["","","","M","kW","0.014","0.014"]
["","Dust collection efficiency","","Turbo","%","89","89"]
["","Deodorizing efficiency (JEM 1467*)","","Turbo","%","95","95"]
["Running current","Air purifying operation","","Low","A","0.10","0.10"]
["","","","High","A","0.22","0.22"]
["","","","Turbo","A","0.48","0.48"]
["","","","Medium","A","0.14","0.14"]
["","","","Silent","A","0.08","0.08"]
["Power supply","Phase","","","","1~","1~"]
["","Name","","","","VM","VM"]
["","Frequency","","","Hz","50/60","50/60"]
["","Voltage","","","V","220-240/220-230","220-240/220-230"]
["Notes","","","","","(1) - Deodorizing efficiency means the combined removal rate of amonia, acetaldehyde and acetic acid after burning five cigarettes in a 1m³ airtight container and running the air purifier at rated air flow for one minute","(1) - Deodorizing efficiency means the combined removal rate of amonia, acetaldehyde and acetic acid after burning five cigarettes in a 1m³ airtight container and running the air purifier at rated air flow for one minute"]
["","","","","","(2) - Sound pressure levels are the average of values measured at 1m away from the front, left, right and top of the unit (this is equal to the value in an anechoic chamber).","(2) - Sound pressure levels are the average of values measured at 1m away from the front, left, right and top of the unit (this is equal to the value in an anechoic chamber)."]
["","","","","","(3) - Other signs: operation switch: stop; air flow rate indicator","(3) - Other signs: operation switch: stop; air flow rate indicator"]
["Power cord","m","","","","2.0","2.0"]