{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","R-PV1/P1"]
[]
[]
[]
[]
["","","","","","R36PEY1K","R42PEY1K","R48PEY1K","R24PEV1K","R30PEV1K"]
["Sound pressure level","Cooling","","Nom.","dBA","","","","57","58"]
["Refrigerant","Charge","","","kg","","","","2.50","3.40"]
["","Type","","","","","","","R-22","R-22"]
["Piping connections","Piping length","OU - IU","Max.","m","","","","30","30"]
["","Level difference","IU - OU","Max.","m","30","30","30","15","15"]
["Dimensions","Unit","","Width","mm","1,018","1,107","1,107","1,018","980"]
["","","","Depth","mm","412","440","440","412","427"]
["","","","Height","mm","840","1,100","1,100","695","790"]
["Compressor","Type","","","","","","","Rotary","Rotary"]
["Weight","Unit","","","kg","89","94","107","66","73"]
["Power supply","Phase","","","","","","","1~","1~"]
["","Frequency","","","Hz","","","","50","50"]
["","Voltage","","","V","","","","220-240","220-240"]
["Sound pressure level","Cooling","","Nom.","dBA","58","59","59"]
["Refrigerant","Charge","","","kg","3.60","3.05","5.00"]
["","Type","","","","R-22","R-22","R-22"]
["Compressor","Type","","","","Scroll compressor","Scroll compressor","Scroll compressor"]
["Power supply","Phase","","","","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415"]