{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":11,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RD-JV1/JY1"]
[]
[]
[]
[]
["","","","","RD20JEV1K","RD25JEV1K","RD30JEV1K","RD40JEV1K","RD40JEY1K","RD50JEY1K","RD60JEY1K"]
["Sound pressure level","Cooling","Nom.","dBA","52","52","56","68","68","67","66"]
["Refrigerant","Charge","","kg","1.45","1.60","2.10","1.80","1.80","2.60","4.25"]
["","Type","","","R-22","R-22","R-22","R-22","R-22","R-22","R-22"]
["Dimensions","Unit","Width","mm","855","855","855","1,030","1,030","1,030","1,030"]
["","","Depth","mm","328","328","328","400","400","400","400"]
["","","Height","mm","651","753","753","852","852","852","852"]
["Compressor","Type","","","Rotary","Rotary","Twin rotary","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor"]
["Weight","Unit","","kg","47","57","70","88","88","105","108"]
["Power supply","Phase","","","1~","1~","1~","1~","3~","3~","3~"]
["","Frequency","","Hz","50","50","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","380-415","380-415","380-415"]
["Notes","","","","(1) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","","","","(1) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit).","(1) - All units are being tested and comply to ISO 5151 (non-conducted unit) or ISO 1325 (ducted unit)."]
["","","","","","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)","","","(1) - All units are being tested and comply to ISO 5151 (Non-ducted unit)"]
["","","","","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","","","(2) - All specifications are subjected to change by the manufacturer without prior notice."]