{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RKM-PVM"]
[]
[]
[]
[]
["","","","","","RKM18PVMK","RKM24PVMK","RKM28PVMK"]
["Sound pressure level","Cooling","","High","dBA","51","56","57"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","0.8","0.9","1.1"]
["","GWP","","","","675","675","675"]
["","Charge","","","kg","1.12","1.40","1.60"]
["","Type","","","","R-32","R-32","R-32"]
["Fan motor","Speed","Cooling","Super low","rpm","750","800","800"]
["Piping connections","Level difference","IU - OU","Max.","m","20","20","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","930","930","930"]
["","","","Depth","mm","350","350","350"]
["","","","Height","mm","695","695","695"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","46","49","49"]
["Fan","Air flow rate","Cooling","Super low","cfm","2,189","2,168","2,168"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220-230","220-240/220-230","220-240/220-230"]
["Notes","","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]