{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RU-K5"]
[]
[]
[]
[]
["","","","","","RU06KY1","RU08KY1","RU10KY1","RU08KY1+RU08KY1","RU10KY1+RU10KY1"]
["Sound pressure level","Cooling","","Nom.","dBA","59","60","61","60","61"]
["Refrigerant","Charge","","","kg","3.0","5.0","6.1","5.0","6.1"]
["","Type","","","","R-22","R-22","R-22","R-22","R-22"]
["Operation range","Cooling","Ambient","Max.","°CDB","52","52","52"]
["","","","Min.","°CDB","21","21","21"]
["Piping connections","Level difference","IU - IU","Max.","m","30","30","30"]
["Capacity control step","%","","","","100-0","100-0"]
["Dimensions","Unit","","Width","mm","880","1,280","1,280","1,280","1,280"]
["","","","Depth","mm","320","690","690","690","690"]
["","","","Height","mm","1,345","1,220","1,440","1,220","1,440"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","112","177","190","177","190"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415","380-415"]
["Piping connections","Level difference","IU - IU","Max.","m","","","","30","30"]
["Notes","","","","","","","","(1) - Each value for outdoor unit shows the specification per one unit","(1) - Each value for outdoor unit shows the specification per one unit"]