{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RY-CV1"]
[]
[]
[]
[]
["","","","","","RY30CV1M","RY40CV1M","RY60CV1M","RY71CV1M","RY80CV1M","RY90CV1M","RY100CV1M","RY125CV1M"]
["Refrigerant","Charge","","","kg","","0.60","1.35","1.50","2.40","2.15","2.60","2.60"]
["","Type","","","","","R-22","R-22","R-22","R-22","R-22","R-22","R-22"]
["Piping connections","Piping length","OU - IU","Max.","m","","12","15","15","15","45","45","45"]
["","Level difference","IU - OU","Max.","m","5","5","8","8","8","25","25","25"]
["","Additional refrigerant charge","","","kg/m","Depending on distance (see manual)","Depending on distance (see manual)","Depending on distance (see manual)","Depending on distance (see manual)","Depending on distance (see manual)","Depending on distance (see manual)","Depending on distance (see manual)","Depending on distance (see manual)"]
["Dimensions","Unit","","Width","mm","700","700","855","855","855","1,030","1,030","1,030"]
["","","","Depth","mm","250","250","328","328","328","400","400","400"]
["","","","Height","mm","540","540","648","750","750","850","850","850"]
["Compressor","Type","","","","","Rotary","Rotary","Rotary","Rotary","Scroll compressor","Scroll compressor","Scroll compressor"]
["Weight","Unit","","","kg","32","32","59","62","68","95","95","100"]
["Power supply","Phase","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","","50","50","50","50","50","50","50"]
["","Voltage","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 230V","(1) - 230V","(1) - 230V","(1) - 230V","(1) - 230V","(1) - 230V","(1) - 230V","(1) - 230V"]
["Refrigerant","Charge","","","kg","0.63"]
["","Type","","","","R-22"]
["Compressor","Type","","","","Rotary"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]