{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RY-H"]
[]
[]
[]
[]
["","","","","","RY18HEV1K","RY24HEV1K","RY28HEV1K"]
["Sound pressure level","Heating","","Nom.","dBA","52","53","61"]
["","Cooling","","Nom.","dBA","52","53","61"]
["Refrigerant","Charge","","","kg","1.17","1.90","2.55"]
["","Type","","","","R-22","R-22","R-22"]
["Piping connections","Level difference","IU - OU","Max.","m","10","10","15"]
["Dimensions","Unit","","Width","mm","913","955","1,080"]
["","","","Depth","mm","378","396","412"]
["","","","Height","mm","680","700","840"]
["Compressor","Type","","","","Rotary","Rotary","Rotary"]
["Weight","Unit","","","kg","46","55","90"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]