{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RY-HL"]
[]
[]
[]
[]
["","","","","","RY18HEVLK","RY24HEVLK","RY30HEVLK"]
["Sound pressure level","Heating","","Nom.","dBA","52","53","53"]
["","Cooling","","Nom.","dBA","51","52","52"]
["Refrigerant","Charge","","","kg","1.30","1.60","3.00"]
["","Type","","","","R-22","R-22","R-22"]
["Operation range","Cooling","Ambient","Max.","°CDB","52","52","52"]
["","","","Min.","°CDB","18","18","18"]
["","Heating","Ambient","Max.","°CWB","24","24","24"]
["","","","Min.","°CWB","-7","-7","-7"]
["Piping connections","Level difference","IU - OU","Max.","m","10","10","15"]
["Dimensions","Unit","","Width","mm","913","955","950"]
["","","","Depth","mm","378","424","412"]
["","","","Height","mm","680","700","840"]
["Compressor","Type","","","","Rotary","Rotary","Rotary"]
["Weight","Unit","","","kg","46","52","90"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","60","60","60"]
["","Voltage","","","V","220","220","220"]