{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RYD-JVL/JTL/JYL"]
[]
[]
[]
[]
["","","","","RYD20JEVLK","RYD25JEVLK","RYD30JEVLK","RYD40JEVLK","RYD50JETLK","RYD60JETLK"]
["Sound pressure level","Cooling","Nom.","dBA","51","52","57","61","66","66"]
["Refrigerant","Charge","","kg","1.60","1.80","1.75","2.20","2.60","5.00"]
["","Type","","","R-22","R-22","R-22","R-22","R-22","R-22"]
["Dimensions","Unit","Width","mm","855","855","855","1,030","1,030","1,030"]
["","","Depth","mm","328","328","328","400","400","400"]
["","","Height","mm","651","753","756","852","852","852"]
["Compressor","Type","","","Rotary","Rotary","Rotary","Rotary","Rotary","Rotary"]
["Weight","Unit","","kg","49","57","61","81","95","104"]
["Power supply","Phase","","","1~","1~","1~","1~","3~","3~"]
["","Frequency","","Hz","60","60","60","60","60","60"]
["","Voltage","","V","220","220","220","220","220","220"]