{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":10,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RYN-L"]
[]
[]
[]
[]
["","","","","","RYN20LV1B","RYN25LV1B","RYN35LV1B","RYN50LV1B","RYN60LV1B"]
["Refrigerant","Charge","","","TCO2Eq","","1.7"]
["","GWP","","","","","2,087.5"]
["","Charge","","","kg","","0.80"]
["","Type","","","","","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","m","","5"]
["Dimensions","Unit","","Width","mm","","700"]
["","","","Depth","mm","","250"]
["","","","Height","mm","","521"]
["Compressor","Type","","","","","Rotary"]
["Weight","Unit","","","kg","","29"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Notes","","","","","","(1) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","","","(2) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","494","","521","651","753"]
["","","","Width","mm","600","","700","855","855"]
["","","","Depth","mm","245","","250","328","328"]
["Weight","Unit","","","kg","25","","31","49","50"]
["Compressor","Type","","","","Rotary","","Rotary","Rotary","Rotary"]
["Refrigerant","Type","","","","R-410A","","R-410A","R-410A","R-410A"]
["","Charge","","","kg","0.65","","0.85","1.45","1.65"]
["","Charge","","","tCO2Eq","1.7","","1.8","3","3.4"]
["","GWP","","","","2087.5","","2087.5","2087.5","2087.5"]
["Power supply","Phase","","","","1~","","1~","1~","1~"]
["","Frequency","","","Hz","50","","50","50","50"]
["","Voltage","","","V","220-240","","220-240","220-240","220-240"]
["Operation range","Cooling","Ambient","Min.","°CDB","","","19","19","19"]
["","","","Max.","°CDB","","","46","46","46"]
["","Heating","Ambient","Min.","°CWB","","","-9","-9","-9"]
["","","","Max.","°CWB","","","18","18","18"]
["Piping connections","Piping length","OU - IU","Max.","m","","","12","15","15"]
["","Level difference","IU - OU","Max.","m","","","5","8","8"]