{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-KVJ"]
[]
[]
[]
[]
["","","","","","RZQ20KCVJK","RZQ24KCVJK","RZQ36KCVJK","RZQ45KCVJK"]
["Refrigerant","GWP","","","","1,975","1,975","1,975","1,975"]
["","Charge","","","kg","2.75","2.75","3.7","3.7"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Liquid","","OD","mm","9.52","9.52","9.52","9.52"]
["","Piping length","OU - IU","Max.","m","50","50","70","70"]
["","","System","Chargeless","m","30","30","30","30"]
["","","","Equivalent","m","70","70","90","90"]
["","Gas","","OD","mm","15.9","15.9","15.9","15.9"]
["","Level difference","IU - OU","Max.","m","30","30","30","30"]
["Dimensions","Unit","","Width","mm","900","900","900","900"]
["","","","Depth","mm","320","320","320","320"]
["","","","Height","mm","770","770","1,170","1,170"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","68","68","98","98"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","60","60","60","60"]
["","Voltage","","","V","230","230","230","230"]