{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","SEHVX-AAW / SERHQ-AAW1"]
[]
[]
[]
[]
["","","","","SEHVX20AAW / SERHQ020AAW1 (Archived)","SEHVX32AAW / SERHQ032AAW1 (Archived)","SEHVX64AAW / SERHQ032AAW1+SERHQ032AAW1 (Archived)"]
["Cooling capacity","Nom.","","kW","20.7 (3)","30.9 (3)","62.3"]
["Power input","Cooling","Nom.","kW","7.59 (3)","13.5 (3)","27.4"]
["EER","","","","2.73 (3)","2.29 (3)","2.27"]
["Sound power level","Cooling","Nom.","dBA","78","80","83"]
["Energy Efficiency Range","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","(1) - Heating Ta DB/WB 7/6°C - LWC35°C (DT = 5°C), data according EN 14511: 2011","(1) - Heating Ta DB/WB 7/6°C - LWC35°C (DT = 5°C), data according EN 14511: 2011","(1) - Heating Ta DB/WB 7/6°C - LWC35°C (DT = 5°C), data according EN 14511: 2011"]
["","","","","(2) - Heating Ta DB/WB 7/6°C - LWC45°C","(2) - Heating Ta DB/WB 7/6°C - LWC45°C","(2) - Heating Ta DB/WB 7/6°C - LWC45°C"]
["","","","","(3) - Cooling: Ta 35°C - LWE 7°C (DT=5°C), data according EN 14511: 2011","(3) - Cooling: Ta 35°C - LWE 7°C (DT=5°C), data according EN 14511: 2011","(3) - Cooling: Ta 35°C - LWE 7°C (DT=5°C), data according EN 14511: 2011"]
["","","","","(4) - Its functioning relies on fluorinated greenhouse gases","(4) - Its functioning relies on fluorinated greenhouse gases","(4) - Its functioning relies on fluorinated greenhouse gases"]