{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","SEHVX-AAW"]
[]
[]
[]
[]
["","","","","SEHVX20AAW","SEHVX32AAW","SEHVX40AAW","SEHVX64AAW"]
["Casing","Colour","","","Daikin White","Daikin White","Daikin White","Daikin White"]
["","Material","","","Polyester painted galvanised steel plate","Polyester painted galvanised steel plate","Polyester painted galvanised steel plate","Polyester painted galvanised steel plate"]
["Dimensions","Unit","Height","mm","1573","1573","1573","1573"]
["","","Width","mm","766","766","766","766"]
["","","Depth","mm","396","396","396","396"]
["Weight","Unit","","kg","60","62","64","66"]
["Refrigerant","Type","","","R-410A","R-410A","R-410A","R-410A"]
["","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Sound power level","Nom.","","dBA","63","63","66","66"]
["Power supply","Name","","","W1","W1","W1","W1"]
["","Phase","","","3N~","3N~","3N~","3N~"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","400","400","400","400"]
["Notes","","","","(1) - Including piping + PHE; excluding expansion vessel","(1) - Including piping + PHE; excluding expansion vessel","(1) - Including piping + PHE; excluding expansion vessel","(1) - Including piping + PHE; excluding expansion vessel"]
["","","","","(2) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(2) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(2) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(2) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required."]
["","","","","(3) - Excluding the water volume in the unit. This volume will guarantee suficient defrost energy for all applications, however, this volume can be multiplied by 0,66 if the heating sepoint is ≥ 45° C (eg. Fan coils)","(3) - Excluding the water volume in the unit. This volume will guarantee suficient defrost energy for all applications, however, this volume can be multiplied by 0,66 if the heating sepoint is ≥ 45° C (eg. Fan coils)","(3) - Excluding the water volume in the unit. This volume will guarantee suficient defrost energy for all applications, however, this volume can be multiplied by 0,66 if the heating sepoint is ≥ 45° C (eg. Fan coils)","(3) - Excluding the water volume in the unit. This volume will guarantee suficient defrost energy for all applications, however, this volume can be multiplied by 0,66 if the heating sepoint is ≥ 45° C (eg. Fan coils)"]
["","","","","(4) - Its functioning relies on fluorinated greenhouse gases","(4) - Its functioning relies on fluorinated greenhouse gases","(4) - Its functioning relies on fluorinated greenhouse gases","(4) - Its functioning relies on fluorinated greenhouse gases"]