{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","UAT-CGXY"]
[]
[]
[]
[]
["","","","","","UAT150CGXY1","UAT180CGXY1","UAT240CGXY1","UAT300CGXY1"]
["Sound pressure level","Cooling","","","dBA","66 (1)","68 (1)","68 (1)","73 (1)"]
["Evaporator piping connections","Condensation drain size","","OD","mm","25.40","25.40","25.40","25.40"]
["Cooling capacity","Nom.","","","kW","43.96 (1), 42.26 (2), 39.21 (3), 38.71 (4)","56.36 (1), 54.25 (2), 50.85 (3), 49.765 (4)","74.74 (1), 71.81 (2), 67.409 (3), 64.478 (4)","92.12 (1), 87.92 (2), 83.47 (3), 81.565 (4)"]
["Power input","Cooling","","Nom.","kW","13.07","16.92","23.00","28.36"]
["Sound power level","Cooling","","","dBA","85","87","87","92"]
["Dimensions","Unit","","Width","mm","1,965","1,965","1,965","2,410"]
["","","","Depth","mm","1,630","1,630","1,905","2,030"]
["","","","Height","mm","1,390","1,390","1,690","1,650"]
["Casing","Colour","","","","Light grey","Light grey","Light grey","Light grey"]
["EER","","","","","1.51 (4)","1.55 (4)","1.62 (4)","1.57 (4)"]
["Condenser","Refrigerant","","Type","","R-22","R-22","R-22","R-22"]
["Evaporator","Supply side","Fan","Nominal ESP","Pa","125","150","200","250"]
["Power supply","Phase","","","","3N~","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415"]
["Notes","","","","","(1) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 35 °C DB outdoor","(1) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 35 °C DB outdoor","(1) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 35 °C DB outdoor","(1) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 35 °C DB outdoor"]
["","","","","","(2) - Cooling capacity based on ARI standard with condition 26.7 °C DB/19.4 °C WB indoor and 35 °C DB outdoor","(2) - Cooling capacity based on ARI standard with condition 26.7 °C DB/19.4 °C WB indoor and 35 °C DB outdoor","(2) - Cooling capacity based on ARI standard with condition 26.7 °C DB/19.4 °C WB indoor and 35 °C DB outdoor","(2) - Cooling capacity based on ARI standard with condition 26.7 °C DB/19.4 °C WB indoor and 35 °C DB outdoor"]
["","","","","","(3) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 46 °C DB outdoor","(3) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 46 °C DB outdoor","(3) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 46 °C DB outdoor","(3) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 46 °C DB outdoor"]
["","","","","","(4) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 48 °C DB outdoor","(4) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 48 °C DB outdoor","(4) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 48 °C DB outdoor","(4) - Gross cooling capacity based on 26.7 °C DB/19.4 °C WB indoor and 48 °C DB outdoor"]
["","","","","","(5) - Gross capacity does not include the effect of evaporator fan motor heat","(5) - Gross capacity does not include the effect of evaporator fan motor heat","(5) - Gross capacity does not include the effect of evaporator fan motor heat","(5) - Gross capacity does not include the effect of evaporator fan motor heat"]
["","","","","","(6) - All specifications are subjected to change by the manufacturer without prior notice.","(6) - All specifications are subjected to change by the manufacturer without prior notice.","(6) - All specifications are subjected to change by the manufacturer without prior notice.","(6) - All specifications are subjected to change by the manufacturer without prior notice."]