{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-A"]
[]
[]
[]
[]
["","","","","ADEA71A2VEB / ARXM71A5V1B"]
["Puissance frigorifique","Nom.","","kW","6.8"]
["","Max.","","kW","6.98"]
["Puissance calorifique","Nom.","","kW","7.5"]
["","Max.","","kW","7.66"]
["Efficacité nominale","EER","","","2.95"]
["","COP","","","3.49"]
["","Consommation énergétique annuelle","","kWh","1153"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","C"]
["","","Chauffage","","B"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A"]
["","Puissance","Pdesign","kW","6.8"]
["","SEER","","","5.35"]
["","Consommation d’énergie annuelle","","kWh/a","445"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A"]
["","Puissance","Pdesign","kW","6"]
["","SCOP/A","","","3.8"]
["","Pdh Puissance calorifique à -10°","","kW","4.83"]
["","Consommation d’énergie annuelle","","kWh/a","2209"]
["Classe d'efficacité énergétique","","","","A+++ ~ D"]
["Remarques","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes: température intérieure: 27°CBS, 19°CBH; température extérieure: 35°CBS ; longueur équivalente de tuyauterie de réfrigérant: 5m, dénivellation: 0m."]
["","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes: température intérieure: 20°CBS; température extérieure: 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente: 5m, dénivelé: 0m."]
["","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","(4) - Pour les données électriques, se reporter au schéma séparé."]