{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","12.10"]
["Puissance calorifique","Puissance totale","","Nom.","kW","13.5"]
["Caisson","Couleur","","","","Blanc frais"]
["Dimensions","Unité","","Hauteur","mm","1850"]
["","","","Largeur","mm","600"]
["","","","Profondeur","mm","350"]
["Poids","Unité","","","kg","50"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","28"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","26"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","24"]
["","","Chauffage","Haut","m³/min","28"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","26"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","24"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","63"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","51"]
["","Refroidissement","","Moyen","dBA","48"]
["","","","Bas","dBA","46"]
["","Chauffage","","Haut","dBA","51"]
["","","","Moyen","dBA","46"]
["","","","Nom.","dBA","48"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52"]
["","Gaz","","DE","mm","15.9"]
["","Évacuation","","","","I.D. 20/O.D. 26"]
["Systèmes de commande","Télécommande câblée","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Accessoires standard","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50/60"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240/220"]