{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M / 2MXM-M"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B / CTXM15M2V1B / 2MXM40M2V1B","CTXM15M2V1B / CTXM15M2V1B / 2MXM40M3V1B","CTXM15M2V1B / CTXM15M2V1B / 2MXM50M2V1B"]
["Puissance frigorifique","Nom.","","kW","3.00","3.0","3.00"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","302 (0.000)","302","310"]
["","EER","","","4.97","4.97","4.84"]
["","COP","","","4.35","4.35","4.58"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A","A"]
["","","Chauffage","","A","A","A"]
["Puissance calorifique","Nom.","","kW","3.50","3.50"]
["","Min.","","kW","","","4.00"]
["Remarques","","","","","(1) - Puissances frigo. nominales basées sur : température int. : 27°CBS, 19°CBH, température ext. : 35°CBS, tuyauterie de réfrig. équiv. : 5 m, diff. de niveau : 0 m. Données pour séries d'effic. standard"]
["","","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["","","","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]