{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM601A51"]
[]
[]
[]
[]
["","","","","DCM601A51."]
["Température extérieure","Humidité relative <","","%","85"]
["Nombre maximum d'unités intérieures connectables","","","","64, 512 (1), 2,560 (2)"]
["Puissance absorbée","kW","","","0.023"]
["Communication","DIII-NET","Quantité","","1"]
["","Ethernet","Remarque","","Accès Web (100BASE-TX)"]
["","","Quantité","","1"]
["","Modem","Remarque","","Système d'entretien de réseau de climatisation"]
["Installation","","","","Direction verticale uniquement"]
["Dimensions","Unité","Largeur","mm","290"]
["","","Profondeur","mm","50"]
["","","Hauteur","mm","243"]
["Poids","Unité","","kg","2.4"]
["Power supply","Fréquence","","Hz","50/60"]
["","Tension","","V","AC 100-240"]
["Remarques","","","","(1) - Avec 7 adaptateurs ITM Plus"]
["","","","","(2) - Avec 5 ITM combinés avec intégrateur ITM"]