{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Entrée","Type","","","","Écran tactile (entrée analogique codée 10 bits)"]
["Température extérieure","Humidité relative <","","","%","85"]
["","Fonctionnement","","Min.","°C","0"]
["","","","Max.","°C","40"]
["Nombre maximum d'unités intérieures connectables","","","","","64, 128 (1)"]
["Communication","DIII-NET","","Quantité","","1"]
["","","","Remarque","","Ligne de communication de l'équipement de climatisation"]
["","10BASE-T","","Remarque","","Option Web"]
["","Ethernet","","Remarque","","Port pour accès Web et fonction de messagerie électronique"]
["","Borne d’entrée","Numérique","Quantité","","1"]
["","","","Remarque","","Arrêt forcé"]
["","","Impulsion","Quantité","","3"]
["","","","Remarque","","Impulsion de mesure de puissance"]
["","Modem","","Remarque","","Capacité de modem intégré"]
["","PCMCIA","","Remarque","","Carte mémoire Flash"]
["","RS-232C","","Remarque","","Adaptateur DIII-NET-Plus"]
["Dimensions","Unité","","Largeur","mm","230"]
["","","","Profondeur","mm","107"]
["","","","Hauteur","mm","147"]
["Écran LCD","Type","","","","QVGA (320 x 240), 4 096 couleurs"]
["","Dimensions","","Largeur","pouce","5.7"]
["Nombre maximum d'unités extérieures connectables","","","","","10, 20 (1)"]
["Power supply","Fréquence","","","Hz","50/60"]
["","Tension","","","V","100-240 (alimentation externe)"]
["Remarques","","","","","(1) - En combinaison avec DCS601A51"]