{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":16,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-CB / ERLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHVH04S18CB3V / ERLQ004CAV3","EHVH08S18CB3V / ERLQ006CAV3","EHVH08S26CB9W / ERLQ006CAV3","EHVH08S26CB9W / ERLQ008CAV3","EHVH08S18CB3V / ERLQ008CAV3","EHVH11S18CB3V / ERLQ011CAV3","EHVH11S26CB9W / ERLQ011CAV3","EHVH16S26CB9W / ERLQ014CAV3","EHVH16S18CB3V / ERLQ014CAV3","EHVH16S26CB9W / ERLQ016CAV3","EHVH16S18CB3V / ERLQ016CAV3"]
["Production d'eau chaude sanitaire","Général","","Profil de charge déclaré","","L","L","XL","","","L","XL","XL","L","XL","L"]
["","Climat moyen","","Classe","","A","A","A","","","A","A","A","A","A","A"]
["COP","","","","","5.04 (1), 3.58 (2)","4.74 (1), 3.56 (2)","4.74 (1), 3.56 (2)","4.45, 3.42","4.45, 3.42","4.60 (1), 2.75 (3), 3.55 (2), 2.10 (4)","4.60 (1), 2.75 (3), 3.55 (2), 2.10 (4)","4.30 (1), 2.65 (3), 3.32 (2), 2.08 (4)","4.30 (1), 2.65 (3), 3.32 (2), 2.08 (4)","4.25 (1), 2.64 (3), 3.26 (2), 2.09 (4)","4.25 (1), 2.64 (3), 3.26 (2), 2.09 (4)"]
["Puissance calorifique","Nom.","","","kW","4.40 (1), 4.03 (2)","6.00 (1), 5.67 (2)","6.00 (1), 5.67 (2)","","","11.2 (1), 11.0 (2)","11.2 (1), 11.0 (2)","14.5 (1), 13.6 (2)","14.5 (1), 13.6 (2)","16.0 (1), 15.2 (2)","16.0 (1), 15.2 (2)"]
["","Min.","","","kW","1.80 (1)","1.80 (1)","1.80 (1)"]
["","Max.","","","kW","5.12 (1), 4.90 (2)","8.35 (1), 7.95 (2)","8.35 (1), 7.95 (2)","","","8.60 (3), 8.60 (4)","8.60 (3), 8.60 (4)","10.6 (3), 10.8 (4)","10.6 (3), 10.8 (4)","11.4 (3), 10.9 (4)","11.4 (3), 10.9 (4)"]
["Puissance absorbée","Chauffage","","Max.","kW","","","","","","3.13 (3), 4.10 (4)","3.13 (3), 4.10 (4)","4.00 (3), 5.19 (4)","4.00 (3), 5.19 (4)","4.32 (3), 5.22 (4)","4.32 (3), 5.22 (4)"]
["","","","Nom.","kW","0.870 (1), 1.13 (2)","1.27 (1), 1.59 (2)","1.27 (1), 1.59 (2)","","","2.43 (1), 3.10 (2)","2.43 (1), 3.10 (2)","3.37 (1), 4.10 (2)","3.37 (1), 4.10 (2)","3.76 (1), 4.66 (2)","3.76 (1), 4.66 (2)"]
["Remarques","","","","","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)"]
["","","","","","(3) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(3) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(3) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C"]
["","","","","","(4) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(4) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(4) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(4) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C"]
["","","","","","(5) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(5) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(5) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","","","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)"]
["","","","","","(6) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(6) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(6) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","","","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)"]
["","","","","","","","","","","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)"]
["","","","","","","","","","","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","","kW","","","","1.80","1.80"]
["","Nom.","","","kW","","","","7.40, 6.89","7.40, 6.89"]
["","Max.","","","kW","","","","10.0, 9.53","10.0, 9.53"]
["Puissance absorbée","Chauffage","","Nom.","kW","","","","1.66, 2.01","1.66, 2.01"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","","","","XL","L"]
["","Climat moyen","","Classe","","","","","A","A"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-SCOP","","","","","3.20","3.20"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","","","","A++","A++"]
["","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-SCOP","","","","","4.35","4.35"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","","","","A++","A++"]