{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":11,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-CB3V / ERLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHVZ04S18CB3V / ERLQ004CAV3","EHVZ08S18CB3V / ERLQ006CAV3","EHVZ08S18CB3V / ERLQ008CAV3","EHVZ16S18CB3V / ERLQ011CAV3","EHVZ16S18CB3V / ERLQ014CAV3","EHVZ16S18CB3V / ERLQ016CAV3"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","","","L"]
["","Climat moyen","","Classe","","","","A"]
["COP","","","","","5.04, 3.58","4.74, 3.56","4.45 (1), 3.42 (2)","4.60, 2.75, 3.55, 2.10","4.24, 2.61, 3.28, 2.05","4.22, 2.61, 3.23, 2.07"]
["Puissance calorifique","Nom.","","","kW","","","7.40 (1), 6.89 (2)"]
["","Min.","","","kW","","","1.80 (1)"]
["","Max.","","","kW","","","10.0 (1), 9.53 (2)"]
["Puissance absorbée","Chauffage","","Nom.","kW","","","1.66 (1), 2.01 (2)"]
["Remarques","","","","","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)"]
["","","","","","(3) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(3) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7°C (HR : 85%) - LWC 35°C","(3) - Condition 3 : chauffage Ta BS -7°C (HR : 85%) - LWC 35°C","(3) - Condition 3 : chauffage Ta BS -7°C (HR : 85%) - LWC 35°C"]
["","","","","","(4) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(4) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7°C (HR : 85%) - LWC 45°C","(4) - Condition 4 : chauffage Ta BS -7°C (HR : 85%) - LWC 45°C","(4) - Condition 4 : chauffage Ta BS -7°C (HR : 85%) - LWC 45°C"]
["","","","","","","","(5) - La capacité doit être répartie entre zone principale et zone supplémentaire. Se reporter aux données de PSE pour plus de détails sur la hauteur disponible (kPa).","","(5) - La capacité doit être répartie entre zone principale et zone supplémentaire. Se reporter aux données de PSE pour plus de détails sur la hauteur disponible (kPa).","(5) - La capacité doit être répartie entre zone principale et zone supplémentaire. Se reporter aux données de PSE pour plus de détails sur la hauteur disponible (kPa)."]
["","","","","","","","(6) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)"]
["","","","","","","","(7) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)"]
["","","","","","","","(8) - 15°C-25 °C : BUH uniquement, pas de fonctionnement pompe à chaleur = pendant la mise en service"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","","kW","1.80","1.80"]
["","Nom.","","","kW","4.40, 4.03","6.00, 5.67","","11.2, 11.0","14.4, 13.5","15.9, 15.1"]
["","Max.","","","kW","5.12, 4.90","8.35, 7.95","","8.60, 8.60","10.5, 10.7","11.3, 10.8"]
["Puissance absorbée","Chauffage","","Nom.","kW","0.870, 1.13","1.27, 1.59","","2.43, 3.10","3.39, 4.12","3.77, 4.67"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","L","L","","L","L","L"]
["","Climat moyen","","Classe","","A","A","","A","A","A"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général-=-SCOP","","3.20","3.22","","3.09","3.16","3.06"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A++","A++","","A+","A+","A+"]
["","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général-=-SCOP","","4.52","4.29","","3.98","3.90","3.80"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré : 35 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A++","A++","","A++","A++","A+"]
["Classe d'efficacité énergétique","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Puissance absorbée","Chauffage","","Max.","kW","","","","3.13, 4.10","4.02, 5.21","4.33, 5.22"]