{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Montage","","","","","Mur","Mur"]
["Caisson","Couleur","","","","Blanc + noir","Blanc + noir"]
["","Matériau","","","","Tôle, Styrolène butadiène acrylonitrile","Tôle, Styrolène butadiène acrylonitrile"]
["Dimensions","Unité","Hauteur","Ballon","mm","1032","1283"]
["","","","Largeur","mm","510","510"]
["","","","Profondeur","mm","570","570"]
["Poids","Unité","","Vide","kg","43","47"]
["Réservoir","Volume d'eau","","","l","89","118"]
["","Matériau","","","","Acier émaillé conforme DIN4753TL2","Acier émaillé conforme DIN4753TL2"]
["Ballon","Température d'eau maximum","","","°C","75.0","75.0"]
["Réservoir","Étiquette énergie","","","","B","C"]
["Échangeur de chaleur","Eau chaude sanitaire","","Quantité","","1","1"]
["","","","Matériau du tuyau","","Aluminium","Aluminium"]
["","","","Pression de service","bar","42","42"]
["Chauffage d'appoint","Puissance","","","kW","1.2","1.2"]