{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYT-CZI / EWYT-CZO"]
[]
[]
[]
[]
["","","","","","EWYT021CZI-A1 / EWYT021CZO-A1","EWYT032CZI-A1 / EWYT032CZO-A1","EWYT040CZI-A1 / EWYT040CZO-A1","EWYT064CZI-A2 / EWYT064CZO-A2"]
["Puissance calorifique","Nom.","","","kW","19.93","32.082","38.996","61.816"]
["Puissance frigorifique","Nom.","","","kW","21.13","32.70","39.93","64.41"]
["Puissance absorbée","Chauffage","","Nom.","kW","5.81","9.32","11.73","19.21"]
["","Rafraîchissement","","Nom.","kW","6.56","10.28","13.33","21.86"]
["COP","","","","","3.433","3.442","3.325","3.218"]
["EER","","","","","3.221","3.181","2.995","2.946"]
["SEER","","","","","5.41","5.70","5.36","5.34"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-SCOP","","4.19","4.18","4.18","4.01"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A++","A++","A++","A++"]