{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / AZQS-BY1"]
[]
[]
[]
[]
["","","","","FCAG125BVEB / AZQS125B7Y1B"]
["Puissance frigorifique","Nom.","","kW","12.1 (1)"]
["Puissance calorifique","Nom.","","kW","13.5 (2)"]
["Efficacité nominale","EER","","","2.22 (3)"]
["","COP","","","3.41 (3)"]
["Rafraîchissement de l'air ambiant","Puissance","Pdesign","kW","12.1"]
["","SEER","","","5.16"]
["","Consommation d’énergie annuelle","","kWh/a","1,406"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","7.78"]
["","SCOP/A","","","3.67"]
["","Consommation d’énergie annuelle","","kWh/a","2,969"]
["Remarques","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m"]
["","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m"]
["","","","","(3) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]