{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQSG71L3V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L8V1B","FCQG50FVEB / FCQG50FVEB / RZQSG100L8V1B","FCQG100FVEB / RZQSG100L8V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L8V1B","FCQG125FVEB / RZQSG125L8V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L8V1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L8V1B","FCQG140FVEB / RZQSG140L7V1B"]
["Puissance frigorifique","Nom.","","kW","","","","9.5","","12.0","","","13.4"]
["Rafraîchissement des locaux","SEER","","","5.10","5.10","5.10","6.50","4.80","5.30","4.80","4.80"]
["","Consommation d’énergie annuelle","","kWh/a","467","652","652","511.538","875","792.453","875","875"]
["","Puissance","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Classe d’efficacité énergétique","","","A","A","A","A++","B","A","B","B"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","6.00","7.60","7.60","7.60","7.60","8.03","7.60","7.60"]
["","SCOP/A","","","3.80","3.80","3.80","4.10","3.80","4.01","3.80","3.80"]
["","Classe d’efficacité énergétique","","","A","A","A","A+","A","A+","A","A"]
["","Consommation d’énergie annuelle","","kWh/a","2,211","2,800","2,800","2,595.122","2,800","2,803.491","2,800","2,800"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","","","1,440","","1,870"]
["","EER","","","","","","3.30","","3.21","","","3.01"]
["","COP","","","","","","3.54","","3.41","","","3.41"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","","","A","","A"]
["","","Chauffage","","","","","B","","B"]
["Puissance calorifique","Nom.","","kW","","","","10.8","","13.5","","","15.5"]
["Remarques","","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]