{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Caisson","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","260","260","260","260"]
["","","","Largeur","mm","575","575","575","575"]
["","","","Profondeur","mm","575","575","575","575"]
["Poids","Unité","","","kg","16.0","16.0","17.5","17.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","9.0","10.0","12.0","14.5"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8.0","8.5","10.0","12.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6.5","6.5","7.5","9.5"]
["","","Chauffage","Haut","m³/min","9.0","10.0","12.0","14.5"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.0","8.5","10.0","12.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.5","6.5","7.5","9.5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","48","51","56","60"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","31.0","34.0","39.0","43.0"]
["","Refroidissement","","Moyen","dBA","28.5","30.5","34.0","40.0"]
["","","","Bas","dBA","25.0","25.0","27.0","32.0"]
["","Chauffage","","Haut","dBA","31.0","34.0","39.0","43.0"]
["","","","Moyen","dBA","28.5","30.5","34.0","40.0"]
["","","","Bas","dBA","25.0","25.0","27.0","32.0"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.52","9.52","12.70","12.70"]
["","Évacuation","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Panneau décoratif","Modèle","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Couleur","","","","Blanc (N9.5)","Blanc (N9.5)","Blanc (N9.5)","Blanc (N9.5)"]
["","Dimensions","","Hauteur","mm","46","46","46","46"]
["","","","Largeur","mm","620","620","620","620"]
["","","","Profondeur","mm","620","620","620","620"]
["","Poids","","","kg","2.8","2.8","2.8","2.8"]
["Panneau décoratif&nbsp;2","Panneau décoratif&nbsp;2-=-Modèle","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Panneau décoratif&nbsp;2-=-Couleur","","","","Argent","Argent","Argent","Argent"]
["","Panneau décoratif&nbsp;2-=-Dimensions","","Panneau décoratif&nbsp;2-=-Dimensions-=-Hauteur-=-mm","mm","46","46","46","46"]
["","","","Panneau décoratif&nbsp;2-=-Dimensions-=-Largeur-=-mm","mm","620","620","620","620"]
["","","","Panneau décoratif&nbsp;2-=-Dimensions-=-Profondeur-=-mm","mm","620","620","620","620"]
["","Panneau décoratif&nbsp;2-=-Poids-=-kg","","","kg","2.8","2.8","2.8","2.8"]
["Panneau décoratif&nbsp;3","Panneau décoratif&nbsp;3-=-Modèle","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Panneau décoratif&nbsp;3-=-Couleur","","","","Blanc (RAL9010)","Blanc (RAL9010)","Blanc (RAL9010)","Blanc (RAL9010)"]
["","Panneau décoratif&nbsp;3-=-Dimensions","","Panneau décoratif&nbsp;3-=-Dimensions-=-Hauteur-=-mm","mm","55","55","55","55"]
["","","","Panneau décoratif&nbsp;3-=-Dimensions-=-Largeur-=-mm","mm","700","700","700","700"]
["","","","Panneau décoratif&nbsp;3-=-Dimensions-=-Profondeur-=-mm","mm","700","700","700","700"]
["","Panneau décoratif&nbsp;3-=-Poids-=-kg","","","kg","2.7","2.7","2.7","2.7"]
["Panneau décoratif&nbsp;4","Panneau décoratif&nbsp;4-=-Modèle","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Panneau décoratif&nbsp;4-=-Couleur","","","","BLANC (RAL9010)","Blanc (RAL9010)","Blanc (RAL9010)","Blanc (RAL9010)"]
["","Panneau décoratif&nbsp;4-=-Dimensions","","Panneau décoratif&nbsp;4-=-Dimensions-=-Hauteur-=-mm","mm","55","55","55","55"]
["","","","Panneau décoratif&nbsp;4-=-Dimensions-=-Largeur-=-mm","mm","700","700","700","700"]
["","","","Panneau décoratif&nbsp;4-=-Dimensions-=-Profondeur-=-mm","mm","700","700","700","700"]
["","Panneau décoratif&nbsp;4-=-Poids-=-kg","","","kg","2.7","2.7","2.7","2.7"]
["Systèmes de commande","Télécommande infrarouge","","","","BRC7EB530 (panneau standard ), BRC7F530W (panneau blanc), BRC7F5305 (panneau gris)","BRC7EB530 (panneau standard ), BRC7F530W (panneau blanc), BRC7F5305 (panneau gris)","BRC7EB530 (panneau standard ), BRC7F530W (panneau blanc), BRC7F5305 (panneau gris)","BRC7EB530 (panneau standard ), BRC7F530W (panneau blanc), BRC7F5305 (panneau gris)"]
["","Télécommande câblée","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Accessoires standard","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240"]