{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","39","40","41","","46"]
["","","","Moyen","dBA","32","33","33","","42"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19","19","","24"]
["","","","Bas","dBA","25","25","25","","33"]
["","Rafraîchissement","","Moyen","dBA","32","33","33","","39"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19","19","","24"]
["","","","Bas","dBA","25","25","25","","31"]
["","","","Haut","dBA","39","40","41","","46"]
["Accessoires standard","Manuel d'installation","","","","1","1","1","","1"]
["","Manuel d’utilisation","","","","1","1","1","","1"]
["","Filtre à air","","","","2","2","2","","2"]
["","Télécommande infrarouge","","","","1","1","1","","1"]
["","Plaque de montage de télécommande","","","","1","1","1","","1"]
["","Sachet de vis","","","","1","1","1","","1"]
["","Cache de vis","","","","1","1","1","","1"]
["","Piles sèches AAA","","","","2","2","2","","2"]
["","Précautions générales de sécurité","","","","1","1","1","","1"]
["Réfrigérant","PRP","","","","675.0","675.0","675.0","","675.0"]
["Systèmes de commande","Télécommande câblée","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","","6.35"]
["","Gaz","","DE","mm","9.50","9.50","9.50","","12.70"]
["","Évacuation","","","","18","18","18","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Chauffage","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Sound power level","Rafraîchissement","","","dBA","57","57","60","","60"]
["Dimensions","Unité","","Largeur","mm","798","798","798","","798"]
["","","","Profondeur","mm","189","189","189","","189"]
["","","","Hauteur","mm","295","295","295","","295"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","","Blanc"]
["Poids","Unité","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Moyen","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Bas","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.5","4.5","4.5","","5.7"]
["","","Rafraîchissement","Bas","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Moyen","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Haut","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Phase","","","","1~","1~","1~","","1~"]
["","Nom","","","","V1","V1","V1","","V1"]
["","Fréquence","","","Hz","50","50","50","","50"]
["","Tension","","","V","220-240","220-240","220-240","","220-240"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","","","0.028"]
["","Chauffage","","Nom.","kW","","","","0.036"]
["Caisson","Couleur","","","","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","","","295"]
["","","","Largeur","mm","","","","798"]
["","","","Profondeur","mm","","","","189"]
["Poids","Unité","","","kg","","","","11.50"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","","","13.1"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","","","9.8"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","","","7.2"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","","4.6"]
["","","Chauffage","Haut","m³/min","","","","14.6"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","","","10.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","","","7.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","","5.2"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","","","60"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","","","45"]
["","Refroidissement","","Moyen","dBA","","","","37"]
["","","","Bas","dBA","","","","29"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","","21"]
["","Chauffage","","Haut","dBA","","","","45"]
["","","","Moyen","dBA","","","","37"]
["","","","Bas","dBA","","","","29"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","","21"]
["Réfrigérant","Réfrigérant-=-PRP","","","","","","","675.0"]
["Raccords de tuyauterie","Liquide","","DE","mm","","","","6.35"]
["","Gaz","","DE","mm","","","","12.70"]
["","Évacuation","","","","","","","18"]
["Systèmes de commande","Télécommande infrarouge","","","","","","","ARC466A58"]
["","Télécommande câblée","","","","","","","BRC073"]
["Accessoires standard","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Filtre à air","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Alimentation électrique","Nom","","","","","","","V1"]
["","Phase","","","","","","","1~"]
["","Fréquence","","","Hz","","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","","","220-240"]