{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXN-J"]
[]
[]
[]
[]
["","","","","","FTXN25JEV1B","FTXN35JEV1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","40","41"]
["","","","Faible niveau sonore de fonctionnement","dBA","25","26"]
["","","","Bas","dBA","28","29"]
["","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","22","23"]
["","","","Bas","dBA","26","27"]
["","","","Haut","dBA","40","41"]
["","","","Nom.","dBA","34","35"]
["","Rafraîchissement","","Nom.","dBA","33","34"]
["Accessoires standard","Télécommande infrarouge","","","","1","1"]
["","Manuel d'installation","","","","1","1"]
["","Manuel d’utilisation","","","","1","1"]
["","Piles","","","","2","2"]
["","Support de télécommande","","","","1","1"]
["","Plaque de montage","","","","1","1"]
["","Vis de fixation d'unité intérieure","","","","2","2"]
["","Filtre purificateur d'air photocatalytique à apatite de titane","","","","2","2"]
["","Vis de fixation pour plaque de montage","","","","6","6"]
["","Vis de fixation pour télécommande","","","","2","2"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.040","0.040"]
["","Chauffage","","Nom.","kW","0.040","0.040"]
["Sound power level","Rafraîchissement","","","dBA","","55"]
["","Chauffage","","","dBA","","55"]
["Dimensions","Unité","","Largeur","mm","770","770"]
["","","","Profondeur","mm","200","200"]
["","","","Hauteur","mm","283","283"]
["Caisson","Couleur","","","","Blanc","Blanc"]
["Poids","Unité","","","kg","7","7"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","9.8","10.1"]
["","","","Bas","m³/min","6.2","6.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.6","5.9"]
["","","Rafraîchissement","Bas","m³/min","5.3","5.4"]
["","","","Haut","m³/min","9.2","9.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.0","4.4"]
["","","","Nom.","m³/min","8.0","8.3"]
["","","Rafraîchissement","Nom.","m³/min","7.4","7.6"]
["Power supply","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Nom","","","","V1","V1"]
["","Tension","","","V","220-240","220-240"]
["Remarques","","","","","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)"]