{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXG-L"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXG25L2V1B","FVXG35K2V1B / RXG35L2V1B","FVXG50K2V1B / RXG50L2V1B"]
["Puissance frigorifique","Min.","","kW","1.3","1.4","1.7"]
["","Nom.","","kW","2.5","3.5","5.0"]
["","Max.","","kW","3.0","3.8","5.6"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.3","1.4","1.7"]
["","Nom.","","kW","3.4","4.5","5.8"]
["","Max.","","kW","4.5","5.0","8.1"]
["Efficacité nominale","EER","","","4.63","3.72","3.31"]
["","COP","","","4.42","3.75","3.69"]
["","Consommation énergétique annuelle","","kWh","270","470","755"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A","A"]
["","","Chauffage","","A","A","A"]
["Raccords de tuyauterie","Gaz","DE","mm","9.5","9.5","12.7"]
["","Liquide","DE","mm","6.35","6.35","6.35"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++","A++","A"]
["","Puissance","Pdesign","kW","2.50","3.50","5.00"]
["","SEER","","","6.53","6.48","5.41"]
["","Consommation d’énergie annuelle","","kWh/a","134","189","324"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A++","A+","A+"]
["","Puissance","Pdesign","kW","2.80","3.10","4.60"]
["","SCOP/A","","","4.65","4.00","4.18"]
["","Consommation d’énergie annuelle","","kWh/a","842","1087","1543"]
["Remarques","","","","(1) - Rafraîchissement : temp. intérieure 27°CBS,19°CBH; temp. extérieure 35°CBS, 24°CBH","(1) - Rafraîchissement : temp. intérieure 27°CBS,19°CBH; temp. extérieure 35°CBS, 24°CBH","(1) - Rafraîchissement : temp. intérieure 27°CBS,19°CBH; temp. extérieure 35°CBS, 24°CBH"]
["","","","","(2) - Chauffage: temp. intérieure 20°CBS; temp. extérieure 7°CBS, 6°CBH","(2) - Chauffage: temp. intérieure 20°CBS; temp. extérieure 7°CBS, 6°CBH","(2) - Chauffage: temp. intérieure 20°CBS; temp. extérieure 7°CBS, 6°CBH"]