{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXS-L"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXS25L2V1B","FVXS35FV1B / RXS35L2V1B","FVXS50FV1B / RXS50L2V1B"]
["Puissance frigorifique","Min.","","kW","1.3","1.4"]
["","Max.","","kW","3.0","3.8"]
["","Nom.","","kW","2.5","3.5"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.5"]
["","Évacuation","OD","mm","20.0","20.0"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","285","510"]
["","EER","","","4.39","3.43"]
["","COP","","","4.42","3.78"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Puissance calorifique","Nom.","","kW","3.4","4.5"]
["","Min.","","kW","1.3","1.4"]
["","Max.","","kW","4.5","5.0"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - 220V"]
["","","","","(2) - 220V","(2) - 220V","(2) - 230 V"]
["","","","","(3) - 230 V","(3) - 230 V","(3) - 240V"]
["","","","","(4) - 240V","(4) - 240V"]
["","","","","(5) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m","(5) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m"]
["","","","","(6) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m","(6) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["","","","","(7) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(7) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]
["Puissance frigorifique","Min.","","kW","","","1.4"]
["","Nom.","","kW","","","5.0"]
["","Max.","","kW","","","5.6"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","","","1.4"]
["","Nom.","","kW","","","5.8"]
["","Max.","","kW","","","8.1"]
["Efficacité nominale","EER","","","","","3.23"]
["","COP","","","","","3.63"]
["","Consommation énergétique annuelle","","kWh","","","775"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","","A"]
["","","Chauffage","","","","A"]
["Raccords de tuyauterie","Évacuation","DE","mm","","","20"]
["","Gaz","DE","mm","","","12.7"]
["","Liquide","DE","mm","","","6.35"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","","","A+"]
["","Puissance","Pdesign","kW","","","5.00"]
["","SEER","","","","","5.89"]
["","Consommation d’énergie annuelle","","kWh/a","","","297"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","","","A"]
["","Puissance","Pdesign","kW","","","4.20"]
["","SCOP/A","","","","","3.80"]
["","Consommation d’énergie annuelle","","kWh/a","","","1546"]