{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":9,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWF-BF"]
[]
[]
[]
[]
["","","","","","FWF02B5FV1B","FWF03B5FV1B","FWF04B5FV1B","FWF05B5FV1B"]
["Niveau de pression sonore","Bas","","","dBA","26.0","27.0","27.0","32.0"]
["","Haut","","","dBA","31.0","33.0","42.0","47.0"]
["Accessoires standard","Manuel d'installation et d'exploitation","","","","1","1","1","1"]
["","Flexible d'évacuation","","","","1","1","1","1"]
["","Bride pour flexible de vidange","","","","1","1","1","1"]
["","Rondelle pour attache de suspension","","","","8","8","8","8"]
["","Vis","","","","4","4","4","4"]
["","Guide d'installation","","","","1","1","1","1"]
["","Joint torique","","","","4","4","4","4"]
["","Isolation","","","","8","8","8","8"]
["Niveau de puissance sonore totale","Bas","","","dBA","36.0","38.0","41.0","44.0"]
["","Haut","","","dBA","44.0","46.0","52.0","57.0"]
["Débit d'eau","Chute de pression d'eau","Chauffage","Haut","kPa","9","5","9","13"]
["","","Rafraîchissement","Haut","kPa","6","16","26","38"]
["Raccords de tuyauterie","Évacuation","","DE","mm","VP20 (diamètre ext. : 26 / diamètre int. : 20)","VP20 (diamètre ext. : 26 / diamètre int. : 20)","VP20 (diamètre ext. : 26 / diamètre int. : 20)","VP20 (diamètre ext. : 26 / diamètre int. : 20)"]
["","Eau","","Entrée","","3/4\" BSP (filetage femelle)","3/4\" BSP (filetage femelle)","3/4\" BSP (filetage femelle)","3/4\" BSP (filetage femelle)"]
["","","","Sortie","","3/4\" BSP (filetage femelle)","3/4\" BSP (filetage femelle)","3/4\" BSP (filetage femelle)","3/4\" BSP (filetage femelle)"]
["Puissance absorbée","Haut","","","kW","0.074","0.074","0.094","0.121"]
["","Bas","","","kW","0.060","0.055","0.055","0.066"]
["Température d'eau autorisée","Chauffage","","Max.","°C","70 (5)","70 (5)","70 (5)","70 (5)"]
["","","","Min.","°C","5 (5)","5 (5)","5 (5)","5 (5)"]
["","Rafraîchissement","","Min.","°C","5 (5)","5 (5)","5 (5)","5 (5)"]
["","","","Max.","°C","70 (5)","70 (5)","70 (5)","70 (5)"]
["Dimensions","Unité","","Largeur","mm","575","575","575","575"]
["","","","Profondeur","mm","575","575","575","575"]
["","","","Hauteur","mm","285 (4)","285 (4)","285 (4)","285 (4)"]
["Poids","Unité","","","kg","20","20","20","20"]
["Ventilateur","Débit d’air","","Bas","m³/h","318","300","300","390"]
["","","","Haut","m³/h","468","438","618","822"]
["Puissance frigorifique (conditions standards)","Puissance totale (4 tuyaux)","","Bas","kW","1.3 (1)","1.6 (1)","1.6 (1)","2.6 (1)"]
["","","","Haut","kW","1.8 (1)","2.9 (1)","3.8 (1)","4.6 (1)"]
["","Puissance sensible (4 tuyaux)","","Bas","kW","1.0 (1)","1.0 (1)","1.0 (1)","1.6 (1)"]
["","","","Haut","kW","1.5 (1)","1.8 (1)","2.5 (1)","3.2 (1)"]
["Puissance calorifique (conditions standards)","Puissance (4 tuyaux)","","Bas","kW","2.4 (3)","2.6 (3)","2.6 (3)","3.2 (3)"]
["","","","Haut","kW","3.3 (3)","3.6 (3)","4.7 (3)","5.7 (3)"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50"]
["","Tension","","","V","220-440","220-440","220-440","220-440"]
["Remarques","","","","","(1) - Rafraîchissement: air 27 °CBS, 19 °CBH ; eau à l'entrée 7 °C ; eau en sortie 12 °C","(1) - Rafraîchissement: air 27 °CBS, 19 °CBH ; eau à l'entrée 7 °C ; eau en sortie 12 °C","(1) - Rafraîchissement: air 27 °CBS, 19 °CBH ; eau à l'entrée 7 °C ; eau en sortie 12 °C","(1) - Rafraîchissement: air 27 °CBS, 19 °CBH ; eau à l'entrée 7 °C ; eau en sortie 12 °C"]
["","","","","","(2) - Chauffage : 2 tuyaux : air 20°C BS, 15°C BH ; entrée d'eau 45°C ; sortie d’eau 40°C","(2) - Chauffage : 2 tuyaux : air 20°C BS, 15°C BH ; entrée d'eau 45°C ; sortie d’eau 40°C","(2) - Chauffage : 2 tuyaux : air 20°C BS, 15°C BH ; entrée d'eau 45°C ; sortie d’eau 40°C","(2) - Chauffage : 2 tuyaux : air 20°C BS, 15°C BH ; entrée d'eau 45°C ; sortie d’eau 40°C"]
["","","","","","(3) - Chauffage : 4 tuyaux : air 20°C BS, 15°C BH ; entrée d'eau 65°C ; sortie d’eau 55°C","(3) - Chauffage : 4 tuyaux : air 20°C BS, 15°C BH ; entrée d'eau 65°C ; sortie d’eau 55°C","(3) - Chauffage : 4 tuyaux : air 20°C BS, 15°C BH ; entrée d'eau 65°C ; sortie d’eau 55°C","(3) - Chauffage : 4 tuyaux : air 20°C BS, 15°C BH ; entrée d'eau 65°C ; sortie d’eau 55°C"]
["","","","","","(4) - La hauteur inclut le boîtier électrique.","(4) - La hauteur inclut le boîtier électrique.","(4) - La hauteur inclut le boîtier électrique.","(4) - La hauteur inclut le boîtier électrique."]
["","","","","","(5) - Ne pas laisser d'eau à température inférieure à 5 °C ou supérieure à 50/70 °C pénétrer dans l'unité, au risque d'endommager cette dernière.","(5) - Ne pas laisser d'eau à température inférieure à 5 °C ou supérieure à 50/70 °C pénétrer dans l'unité, au risque d'endommager cette dernière.","(5) - Ne pas laisser d'eau à température inférieure à 5 °C ou supérieure à 50/70 °C pénétrer dans l'unité, au risque d'endommager cette dernière.","(5) - Ne pas laisser d'eau à température inférieure à 5 °C ou supérieure à 50/70 °C pénétrer dans l'unité, au risque d'endommager cette dernière."]