{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC707"]
[]
[]
[]
[]
["","","","","","MC707VM-S","MC707VM-W"]
["Niveau de pression sonore","Mode purification","","Haut","dBA","38.0","38.0"]
["","","","Turbo","dBA","47.0","47.0"]
["","","","Moyen","dBA","31.0","31.0"]
["","","","Bas","dBA","24.0","24.0"]
["","","","Silence","dBA","16.0","16.0"]
["Accessoires standard","Télécommande infrarouge","","","","1","Télécommande infrarouge"]
["","Filtre photocatalytique plissé","","","","7","7"]
["","Manuel d’utilisation","","","","1","1"]
["","Filtre antibactérien BIO","","","","1","1"]
["Dispositifs de sécurité","Élément","","01","","Interrupteur de sécurité (arrêt du fonctionnement à l'ouverture du panneau frontal)","Interrupteur de sécurité (arrêt du fonctionnement à l'ouverture du panneau frontal)"]
["Dimensions","Unité","","Largeur","mm","425","425"]
["","","","Profondeur","mm","213","213"]
["","","","Hauteur","mm","533","533"]
["Bacteria filtering method","","","","","Filtre purificateur d'air photocatalytique à apatite de titane, Filtre antibactérien Bio, Flash streamer","Filtre purificateur d'air photocatalytique à apatite de titane, Filtre antibactérien Bio, Flash streamer"]
["Caisson","Couleur","","","","Argent","Blanc"]
["Surface applicable","m²","","","","48","48"]
["Dust collecting method","","","","","Filtre de collecte électrostatique des poussières, Ioniseur plasma (collecte électrostatique des poussières)","Filtre de collecte électrostatique des poussières, Ioniseur plasma (collecte électrostatique des poussières)"]
["Deodorizing method","","","","","Catalyseur désodorisant, Filtre purificateur d'air photocatalytique à apatite de titane, Flash streamer","Catalyseur désodorisant, Flash streamer, Filtre purificateur d'air photocatalytique à apatite de titane"]
["Poids","Unité","","","kg","8.7","8.7"]
["Type","","","","","Purificateur d'air photocatalytique","Purificateur d'air photocatalytique"]
["Ventilateur","Débit d'air","Mode purification","Turbo","m³/h","420","420"]
["","","","Haut","m³/h","285","285"]
["","","","Silence","m³/h","60","60"]
["","","","Bas","m³/h","120","120"]
["","","","Moyen","m³/h","180","180"]
["Contrôle du débit d'air","Mode","","","","5","5"]
["Puissance","m³/min","","","","7.0","7.0"]
["Application","","","","","Type table","Type table"]
["Mode purification","Puissance absorbée","","Turbo","kW","0.055","0.055"]
["","","","Silence","kW","0.008","0.008"]
["","","","L","kW","0.010","0.010"]
["","","","GV","kW","0.023","0.023"]
["","","","M","kW","0.014","0.014"]
["","Efficacité de collecte des poussières","","Turbo","%","89","89"]
["","Efficacité de désodorisation (JEM 1467*)","","Turbo","%","95","95"]
["Courant de fonctionnement","Mode purification","","Bas","A","0.10","0.10"]
["","","","Haut","A","0.22","0.22"]
["","","","Turbo","A","0.48","0.48"]
["","","","Moyen","A","0.14","0.14"]
["","","","Silence","A","0.08","0.08"]
["Power supply","Phase","","","","1~","1~"]
["","Nom","","","","VM","VM"]
["","Fréquence","","","Hz","50/60","50/60"]
["","Tension","","","V","220-240/220-230","220-240/220-230"]
["Remarques","","","","","(1) - L'efficacité de désodorisation est basé sur le taux d'élimination combinée de l'ammoniac, de l'acétaldéhyde et de l'acide acétique produits par la fumée de cinq cigarettes dans un conteneur hermétique de 1 m³ et sur un fonctionnement du purificateur de l'air à débit d'air nominal pendant une minute.","(1) - L'efficacité de désodorisation est basé sur le taux d'élimination combinée de l'ammoniac, de l'acétaldéhyde et de l'acide acétique produits par la fumée de cinq cigarettes dans un conteneur hermétique de 1 m³ et sur un fonctionnement du purificateur de l'air à débit d'air nominal pendant une minute."]
["","","","","","(2) - Les niveaux de pression sonore correspondent à la moyenne des valeurs mesurées à 1 m de distance de l'avant, des côtés gauche et droit, et du dessus de l'unité (équivalent à la valeur en chambre anéchoïque).","(2) - Les niveaux de pression sonore correspondent à la moyenne des valeurs mesurées à 1 m de distance de l'avant, des côtés gauche et droit, et du dessus de l'unité (équivalent à la valeur en chambre anéchoïque)."]
["","","","","","(3) - Autres témoins : interrupteur de fonctionnement : arrêt ; indicateur de débit d'air","(3) - Autres témoins : interrupteur de fonctionnement : arrêt ; indicateur de débit d'air"]
["Cordon d'alimentation","m","","","","2.0","2.0"]