{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","R-H"]
[]
[]
[]
[]
["","","","","","R18HEV1K","R24HEV1K","R28HEV1K"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","52","54","60"]
["Réfrigérant","Charge","","","kg","1.1","1.6","2.7"]
["","Type","","","","R22","R22","R22"]
["Raccords de tuyauterie","Dénivelé","UI - UE","Max.","m","10","10","15"]
["Compresseur","Type","","","","Rotatif","Rotatif","Rotatif"]
["Dimensions","Unité","","Largeur","mm","913","955","950"]
["","","","Profondeur","mm","378","424","412"]
["","","","Hauteur","mm","680","700","840"]
["Poids","Unité","","","kg","45","51","90"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Tension","","","V","220-240","220-240","220-240"]