{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":5,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RDXYQ-TA"]
[]
[]
[]
[]
["","","","","RDXYQ5TAV1B"]
["Niveau de pression sonore","Rafraîchissement","Nom.","dBA","54 (5)"]
["Accessoires standard","Manuel d'installation et d'exploitation","","","1"]
["","Flexible d'évacuation","","","1"]
["","Vis","","","1"]
["","Attaches","","","1"]
["","Collier de serrage","","","1"]
["Poids","Unité","","kg","103"]
["Réfrigérant","Type","","","R-410A"]
["Raccords de tuyauterie","Évacuation","DE","mm","32"]
["Sound power level","Rafraîchissement","Nom.","dBA","81 (4)"]
["Dimensions","Unité","Largeur","mm","1,456"]
["","","Profondeur","mm","1,044"]
["","","Hauteur","mm","397"]
["","Gaine","Hauteur","mm","298"]
["","","Largeur","mm","1,196"]
["Power supply","Phase","","","1N~"]
["","Fréquence","","Hz","50"]
["","Nom","","","V1"]
["","Tension","","V","220-240"]
["Remarques","","","","(1) - Puissances frigo. nominales basées sur : température int. : 27°CBS, 19°CBH, température ext. : 35°CBS, tuyauterie de réfrig. équiv. : 5 m, diff. de niveau : 0 m. Données pour séries d'effic. standard"]
["","","","","(2) - Puissances calo. nominales basées sur : température int. : 20°CBS, température ext. : 7°CBS, 6°CBH, tuyauterie de réfrig. équiv. : 5 m, diff. de niveau : 0 m. Données pour séries d'effic. standard"]
["","","","","(3) - Le nombre réel d'unités dépend du type d'unités intérieures (VRV DX, etc.) et de la limitation du ratio de connexion du système (; 50% ≤ RC ≤ 130%)."]
["","","","","(4) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore."]
["","","","","(5) - Il s'agit d'une valeur relative qui varie en fonction de la distance et de l'environnement acoustique. Pour plus de détails, se reporter aux schémas du niveau sonore. Débit d'air nominal, PSE 60 Pa."]
["","","","","(6) - Se reporter au manuel de sélection de tuyau de réfrigérant ou d'installation"]
["","","","","(7) - Conformément à la norme EN/CEI 61000-3-12, il peut s'avérer nécessaire de prendre contact avec l'opérateur du réseau de distribution d'électricité afin de s'assurer que l'équipement est connecté uniquement à une alimentation avec une valeur Ssc ≥ à la valeur Ssc minimale."]
["","","","","(8) - Les valeurs sonores sont mesurées en salle semi-anéchoïque."]
["","","","","(9) - Contient des gaz à effet de serre fluorés."]