{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXN-L"]
[]
[]
[]
[]
["","","","","","RXN25LV1B","RXN35LV1B (Archived)","RXN50LV1B (Archived)","RXN60LV1B (Archived)"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","48","51","51"]
["Réfrigérant","Charge","","","TCO2Eq","","2.1","3","3.1"]
["","PRP","","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","","1.00","1.45","1.50"]
["","Type","","","","","R-410A","R-410A","R-410A"]
["Compresseur","Type","","","","","Swing hermétique","Swing hermétique","Swing hermétique"]
["Dimensions","Unité","","Largeur","mm","","658","855","855"]
["","","","Profondeur","mm","","289","328","328"]
["","","","Hauteur","mm","","550","753","753"]
["Poids","Unité","","","kg","","30","49","49"]
["Power supply","Phase","","","","","1~","1~","1~"]
["","Fréquence","","","Hz","","50","50","50"]
["","Tension","","","V","","220-240","220-240","220-240"]
["Remarques","","","","","","(1) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis.","(1) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis.","(1) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis."]
["","","","","","","(2) - Contient des gaz à effet de serre fluorés.","(2) - Contient des gaz à effet de serre fluorés.","(2) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","550"]
["","","","Largeur","mm","658"]
["","","","Profondeur","mm","289"]
["Poids","Unité","","","kg","28"]
["Compresseur","Type","","","","Swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","10"]
["","","","Max.","°CBS","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15"]
["","","","Max.","°CBH","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46"]
["Réfrigérant","","","","","R-410A"]
["","Charge","","","kg","0.74"]
["","Charge","","","tCO2Eq","1.5"]
["","Réfrigérant-=-PRP","","","","2087.5"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240"]