{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B","RXS25K2V1B (Archived)"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","47","","47","48","48","48"]
["","Rafraîchissement","","Haut","dBA","46","","46","48","48","48"]
["Accessoires standard","Joint (évacuation)","","","","1","","1"]
["","Manuel d'installation","","","","1","","1","1","1","1"]
["Réfrigérant","Charge","","","TCO2Eq","2.1","","2.1","2.5","2.7","3.5"]
["","PRP","","","","2,087.5","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","","1.0","1.2","1.3","1.7"]
["","Type","","","","R-410A","","R-410A","R-410A","R-410A","R-410A"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","780","","780","780","790","670"]
["","","Chauffage","Très lent","tr/min","740","","740","740","780","670"]
["Raccords de tuyauterie","Dénivelé","UI - UE","Max.","m","15","","15","15","15","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["Compressor","Type","","","","Compresseur swing hermétique","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","765","","765","765","765","825"]
["","","","Profondeur","mm","285","","285","285","285","300"]
["","","","Hauteur","mm","550","","550","550","550","735"]
["Poids","Unité","","","kg","34","","34","34","39","47"]
["Ventil.","Débit d'air","Chauffage","Très lent","cfm","","","","904","960","1,522"]
["","","Rafraîchissement","Extra lent","cfm","","","","1,063","1,080","1,727"]
["Power supply","Phase","","","","1~","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","","50","50","50","50"]
["","Tension","","","V","220-240","","220-240","220-240","220-240","220-240"]
["Remarques","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","","(4) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(4) - Contient des gaz à effet de serre fluorés.","(4) - Contient des gaz à effet de serre fluorés.","(4) - Contient des gaz à effet de serre fluorés."]
["","","","","","(5) - Contient des gaz à effet de serre fluorés.","","(5) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","","550","","","","","550"]
["","","","Largeur","mm","","765","","","","","765"]
["","","","Profondeur","mm","","285","","","","","285"]
["Poids","Unité","","","kg","","34","","","","","34"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","","780","","","","","780"]
["","","Chauffage","Très lent","tr/min","","740","","","","","740"]
["Compressor","Type","","","","","Compresseur swing hermétique","","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","","-10","","","","","-10"]
["","","","Max.","°CBS","","46","","","","","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","","-15","","","","","-15"]
["","","","Max.","°CBH","","18","","","","","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","46","","","","","46"]
["","Chauffage","","Haut","dBA","","47","","","","","47"]
["Réfrigérant","","","","","","R-410A","","","","","R-410A"]
["","Charge","","","kg","","1.0","","","","","1.0"]
["","Charge","","","tCO2Eq","","2.1","","","","","2.1"]
["","Réfrigérant-=-PRP","","","","","2087.5","","","","","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","","20","","","","","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","0,02 (pour longueur de tuyauterie supérieure à 10 m)","","","","","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","","15","","","","","15"]
["Accessoires standard","Installation manual","","","","","1","","","","","1"]
["","Joint (drain)","","","","","1","","","","","1"]
["Alimentation électrique","Phase","","","","","1~","","","","","1~"]
["","Fréquence","","","Hz","","50","","","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240","","","","","220-240"]
["Accessoires standard","Bouchon d'évacuation","","","","","","","1","1","1"]