{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","","48","48","50","50"]
["","Rafraîchissement","","Haut","dBA","","","48","48","49","49"]
["Accessoires standard","Manuel d’utilisation","","","","","","1","1","1","1"]
["","Manuel d'installation","","","","","","1","1","1","1"]
["Réfrigérant","PRP","","","","","","675","675","675","675"]
["","Charge","","","kg","","","1.34","1.34","1.34","1.34"]
["","Type","","","","","","R-32","R-32","R-32","R-32"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Max.","°CBS","","","43","43","43","43"]
["","","","Min.","°CBS","","","-10","-10","-10","-10"]
["","Chauffage","Temp. ext.","Max.","°CBH","","","18","18","18","18"]
["","","","Min.","°CBH","","","-20","-20","-20","-20"]
["Raccords de tuyauterie","Dénivelé","UI - UE","Max.","m","","","8","8","8","8"]
["Dimensions","Unité","","Largeur","mm","","","795","795","795","795"]
["","","","Profondeur","mm","","","300","300","300","300"]
["","","","Hauteur","mm","","","693","693","693","693"]
["Compresseur","Type","","","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Poids","Unité","","","kg","","","50","50","50","50"]
["Power supply","Phase","","","","","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","","","50","50","50","50"]
["","Tension","","","V","","","220-240","220-240","220-240","220-240"]
["Remarques","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","(4) - Contient des gaz à effet de serre fluorés.","(4) - Contient des gaz à effet de serre fluorés.","(4) - Contient des gaz à effet de serre fluorés.","(4) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","693","693"]
["","","","Largeur","mm","795","795"]
["","","","Profondeur","mm","300","300"]
["Poids","Unité","","","kg","50","50"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","43","43"]
["","Chauffage","Temp. ext.","Min.","°CBH","-20","-20"]
["","","","Max.","°CBH","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46","46"]
["","Chauffage","","Haut","dBA","46","46"]
["Réfrigérant","","","","","R-32","R-32"]
["","Charge","","","kg","1.34","1.34"]
["","Charge","","","tCO2Eq","0.9","0.9"]
["","Réfrigérant-=-PRP","","","","675","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","10","10"]
["","Dénivelé","UI - UE","Max.","m","8","8"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]