{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Cooling capacity","Total capacity","","Nom.","كيلوواط","12.10"]
["استطاعة التدفئة","الاستطاعة الإجمالية","","الإسمي","كيلوواط","13.5"]
["الغلاف","اللون","","","","أبيض صاف"]
["الأبعاد","الوحدة","","الارتفاع","mm","1850"]
["","","","العرض","mm","600"]
["","","","العمق","mm","350"]
["الوزن","الوحدة","","","كغ","50"]
["Fan","Air flow rate","التبريد","High","m³/min","28"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","26"]
["Fan","Air flow rate","التبريد","Low","m³/min","24"]
["","","التدفئة","High","m³/min","28"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","26"]
["Fan","Air flow rate","التدفئة","Low","m³/min","24"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","63"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","51"]
["مستوى ضغط الصوت","تبريد","","متوسط","ديسيبل أمبير","48"]
["Sound pressure level","Cooling","","Low","ديسيبل أمبير","46"]
["","Heating","","High","ديسيبل أمبير","51"]
["مستوى ضغط الصوت","تدفئة","","متوسط","ديسيبل أمبير","46"]
["Sound pressure level","Heating","","Nom.","ديسيبل أمبير","48"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52"]
["","غاز","","القطر الخارجي","mm","15.9"]
["","التصريف","","","","I.D. 20/O.D. 26"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["وحدة التزويد بالطاقة","الطور","","","","1~"]
["Power supply","Frequency","","","هرتز","50/60"]
["","Voltage","","","فولت","220-240/220"]