{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":12,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B"]
[]
[]
[]
[]
["","","","","","FCAG35BVEB","FCAG50BVEB","FCAG60BVEB","FCAG71BVEB","FCAG100BVEB","FCAG125BVEB","FCAG140BVEB"]
["Cooling capacity","Total capacity","","Nom.","kW","3.50","5.00","5.70","6.80","9.5","12.1","13.40"]
["استطاعة التدفئة","الاستطاعة الإجمالية","","الإسمي","kW","4.2","6.0","7.0","7.5","10.8","13.5","15.5"]
["الغلاف","المادة","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الأبعاد","الوحدة","","الارتفاع","mm","204","204","204","204","246","246","246"]
["","","","العرض","mm","840","840","840","840","840","840","840"]
["","","","العمق","mm","840","840","840","840","840","840","840"]
["الوزن","الوحدة","","","kg","18","19","19","21","23","23","23"]
["Fan","Air flow rate","Cooling","High","m³/min","12.9","14.6","14.9","15.1","22.7","27.2","27.2"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","10.6","11.8","12.2","13","17.8","20.4","20.4"]
["Fan","Air flow rate","Cooling","Low","m³/min","8.8","9.4","9.6","10.8","13","13.1","13.1"]
["","","Heating","High","m³/min","14.1","14.6","14.9","15.1","23","27","27"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","11.6","11.8","12.2","12.9","18.1","20.2","20.2"]
["Fan","Air flow rate","Heating","Low","m³/min","9.4","9.4","9.6","10.8","13.2","13","13"]
["مستوى طاقة الصوت","التبريد","","","dBA","49","49","51","51","54","58","58"]
["","التدفئة","","","dBA","49","49","51","51","54","58","58"]
["Sound pressure level","Cooling","","High","dBA","31","31","33","35","37","41","41"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","29","29","31","31","33","35","35"]
["Sound pressure level","Cooling","","Low","dBA","27","27","28","28","29","29","29"]
["","Heating","","High","dBA","31","31","33","33","37","41","41"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","29","29","31","31","33","35","35"]
["Sound pressure level","Heating","","Low","dBA","27","27","28","28","29","29","29"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","التصريف","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["لوحة ديكور","الطراز","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","الأبعاد","","الارتفاع","mm","65","65","65","65","65","65","65"]
["","","","العرض","mm","950","950","950","950","950","950","950"]
["","","","العمق","mm","950","950","950","950","950","950","950"]
["","الوزن","","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["لوحة ديكور 2","الطراز","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","الأبعاد","","الارتفاع","mm","148","148","148","148","148","148","148"]
["","","","العرض","mm","950","950","950","950","950","950","950"]
["","","","العمق","mm","950","950","950","950","950","950","950"]
["","الوزن","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["لوحة ديكور 3","الطراز","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","الأبعاد","","الارتفاع","mm","106","106","106","106","106","106","106"]
["","","","العرض","mm","950","950","950","950","950","950","950"]
["","","","العمق","mm","950","950","950","950","950","950","950"]
["","الوزن","","","kg","6.5","6.5","6.5","6.5","6.5","6.5","6.5"]
["أنظمة التحكم","Infrared remote control","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2"]
["","Screws","","","","4","4","4","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1","1","1","1"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~","1~","1~"]
["Power supply","Power supply-=-Frequency","","Frequency","","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Power supply-=-Voltage","","Voltage","","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]