{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RZAG-A"]
[]
[]
[]
[]
["","","","","FNA35A2VEB9 / RZAG35A2V1B","FNA50A2VEB9 / RZAG35A2V1B","FNA50A2VEB9 / RZAG50A2V1B","FNA60A2VEB9 / RZAG50A2V1B","FNA60A2VEB9 / RZAG60A2V1B"]
["Cooling capacity","Min.","","kW","1.6","1.6","1.7","1.7","1.7"]
["","Max.","","kW","4.5","4.5","6.0","6.0","6.5"]
["","Nom.","","kW","3.5","3.5","5.0","5.0","6.0"]
["تبريد المساحة","SEER","","","5.90","6.08","5.90","5.98","5.70"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","208","201","297","293","368"]
["","الاستطاعة","Pdesign","kW","3.50","3.50","5.00","5.00","6.00"]
["","فئة فعالية استهلاك الطاقة","","","A+","A+","A+","A+","A+"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","3.50","4.20","4.30","4.30","4.50"]
["","SCOP/A","","","3.90","4.05","3.90","3.94","3.90"]
["","فئة فعالية استهلاك الطاقة","","","A","A+","A","A","A"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1,255","1,452","1,542","1,528","1,616"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","449","432","658","628","882"]
["","نسبة فعالية استهلاك الطاقة","","","3.90","4.05","3.80","3.98","3.40"]
["","عامل الأداء","","","3.50","3.63","3.40","3.44","3.30"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A"]
["","","تدفئة","","B","A","C","B","C"]
["Heating capacity","Nom.","","kW","4.00","4.00","5.00","5.00","7.00"]
["","Min.","","kW","1.40","1.40","1.70","1.70","1.70"]
["","Max.","","kW","5.00","5.00","6.00","6.00","7.50"]