{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":14,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A"]
[]
[]
[]
[]
["","","","","","FTXF20A5V1B","FTXF20A2V1B","FTXF25A5V1B","FTXF25A2V1B","FTXF35A2V1B","FTXF35A5V1B","FTXF50A2V1B","FTXF60A2V1B","FTXF71A2V1B"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","39","39","40","40","40","40"]
["","","","متوسط","ديسيبل أمبير","34","34","34","34","35","35"]
["","","","Silent operation","ديسيبل أمبير","21","21","21","21","21","21"]
["","","","Low","ديسيبل أمبير","28","28","28","28","29","29"]
["","Cooling","","متوسط","ديسيبل أمبير","33","33","33","33","34","34"]
["","","","Silent operation","ديسيبل أمبير","20","20","20","20","20","20"]
["","","","Low","ديسيبل أمبير","25","25","26","26","27","27"]
["","","","High","ديسيبل أمبير","39","39","40","40","43","43"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1","1","1"]
["","دليل التشغيل","","","","1","1","1","1","1","1"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","1","1","1","1","1","1"]
["","بطاريات جافة قياس AAA","","","","2","2","2","2","2","2"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1","1","1","1"]
["","لوح التثبيت","","","","1","1","1","1","1","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2","2","2","2","2"]
["أنظمة التحكم","Wired remote control","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Piping connections","Liquid","","القطر الخارجي","مم","6.35","6.35","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","مم","9.50","9.50","9.50","9.50","9.50","9.50"]
["","Drain","","","","18","18","18","18","18","18"]
["Power input","Cooling","","Nom.","كيلوواط","0.017","0.017","0.019","0.019","0.032","0.032"]
["","Heating","","Nom.","كيلوواط","0.020","0.020","0.020","0.020","0.032","0.032"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","55","55","55","55","58","58"]
["","التدفئة","","","ديسيبل أمبير","55","55","55","55","58","58"]
["Dimensions","Unit","","العرض","مم","770","770","770","770","770","770"]
["","","","العمق","مم","225","225","225","225","225","225"]
["","","","الارتفاع","مم","286","286","286","286","286","286"]
["الغلاف","اللون","","","","White","White","White","White","White","White"]
["الوزن","الوحدة","","","kg","9.00","9.00","9.00","9.00","9.00","9.00"]
["Fan","Air flow rate","التدفئة","High","م³/دقيقة","10.3","10.3","10.3","10.3","11.5","11.5"]
["","","","Low","م³/دقيقة","6.5","6.5","6.7","6.7","7.0","7.0"]
["","","","متوسط","م³/دقيقة","8.4","8.4","8.6","8.6","9.0","9.0"]
["","","","Silent operation","م³/دقيقة","5.3","5.3","5.3","5.3","5.3","5.3"]
["","","التبريد","Low","م³/دقيقة","5.9","5.9","6.1","6.1","6.3","6.3"]
["","","","متوسط","م³/دقيقة","7.9","7.9","8.1","8.1","8.3","8.3"]
["","","","High","م³/دقيقة","9.8","9.8","10.1","10.1","11.5","11.5"]
["","","","Silent operation","م³/دقيقة","4.4","4.4","4.4","4.4","4.5","4.5"]
["Power supply","الطور","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Power input","Cooling","","Nom.","كيلوواط","","","","","","","0.029","0.032","0.032"]
["","Heating","","Nom.","كيلوواط","","","","","","","0.032","0.035","0.035"]
["الغلاف","اللون","","","","","","","","","","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","مم","","","","","","","295","295","295"]
["","","","العرض","مم","","","","","","","990","990","990"]
["","","","العمق","مم","","","","","","","263","263","263"]
["الوزن","الوحدة","","","kg","","","","","","","13.5","13.5","13.5"]
["Fan","Air flow rate","التبريد","High","م³/دقيقة","","","","","","","16.8","17.3","17.3"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","م³/دقيقة","","","","","","","14.4","14.8","14.8"]
["Fan","Air flow rate","التبريد","Low","م³/دقيقة","","","","","","","11.9","12.2","12.2"]
["","","","Silent operation","م³/دقيقة","","","","","","","10.5","10.7","10.7"]
["","","التدفئة","High","م³/دقيقة","","","","","","","17.3","17.9","17.9"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","م³/دقيقة","","","","","","","14.8","15.8","15.8"]
["Fan","Air flow rate","التدفئة","Low","م³/دقيقة","","","","","","","12.2","12.8","12.8"]
["","","","Silent operation","م³/دقيقة","","","","","","","10.7","11.3","11.3"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","","","","","","","59","60","62"]
["","التدفئة","","","ديسيبل أمبير","","","","","","","61","62","62"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","","","","","","","43","45","46"]
["مستوى ضغط الصوت","تبريد","","متوسط","ديسيبل أمبير","","","","","","","39","41","42"]
["Sound pressure level","Cooling","","Low","ديسيبل أمبير","","","","","","","34","36","37"]
["","","","Silent operation","ديسيبل أمبير","","","","","","","31","33","34"]
["","Heating","","High","ديسيبل أمبير","","","","","","","42","44","45"]
["مستوى ضغط الصوت","تدفئة","","متوسط","ديسيبل أمبير","","","","","","","38","40","41"]
["Sound pressure level","Heating","","Low","ديسيبل أمبير","","","","","","","33","35","36"]
["","","","Silent operation","ديسيبل أمبير","","","","","","","30","32","33"]
["وصلات الأنابيب","سائل","","القطر الخارجي","مم","","","","","","","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","مم","","","","","","","12.7","12.7","12.7"]
["","التصريف","","","","","","","","","","18","18","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","","","","","","","ARC470A1","ARC470A1","ARC470A1"]
["","جهاز تحكم عن بُعد سلكي","","","","","","","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","","","","","","","1","1","1"]
["","AAA dry-cell batteries","","","","","","","","","","2","2","2"]
["","Operation manual","","","","","","","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","","","","","","2","2","2"]
["","Indoor unit fixing screws","","","","","","","","","","2","2","2"]
["","Infrared remote control","","","","","","","","","","1","1","1"]
["","Mounting plate","","","","","","","","","","1","1","1"]
["","Remote control holder","","","","","","","","","","1","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","","","","","","","V1","V1","V1"]
["","الطور","","","","","","","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","","","","","","","50","50","50"]
["","Voltage","","","V","","","","","","","220-240","220-240","220-240"]